# Complementary Filters Shaping Using $\mathcal{H}_\infty$ Synthesis - Matlab Computation
Author: Thomas Dehaeze

UP | HOME

# Complementary Filters Shaping Using \(\mathcal{H}_\infty\) Synthesis - Matlab Computation

## Table of Contents

- 1. H-Infinity synthesis of complementary filters
  - 1.1. Synthesis Architecture
  - 1.2. Design of Weighting Function
  - 1.3. H-Infinity Synthesis
  - 1.4. Obtained Complementary Filters
- 2. Generating 3 complementary filters
  - 2.1. Theory
  - 2.2. Weights
  - 2.3. H-Infinity Synthesis
  - 2.4. Obtained Complementary Filters
- 3. Implement complementary filters for LIGO
  - 3.1. Specifications
  - 3.2. FIR Filter
  - 3.3. Weights
  - 3.4. H-Infinity Synthesis
  - 3.5. Compare FIR and H-Infinity Filters
- 4. Alternative Synthesis
  - 4.1. Two generalized plants
  - 4.2. Shaping the Low pass filter or the high pass filter?
  - 4.3. Using Feedback architecture
  - 4.4. Adding feature in the filters
- 5. Impose a positive slope at DC or a negative slope at infinite frequency
  - 5.1. Manually shift zeros to the origin after synthesis
  - 5.2. Imposing a positive slope at DC during the synthesis phase
  - 5.3. Imposing a negative slope at infinity frequency during the synthesis phase
- 6. Functions
  - 6.1. `generateWF`: Generate Weighting Functions
    - Function description
    - Optional Parameters
    - Generate the Weighting function
    - Verification of the \(G_0\), \(G_c\) and \(G_\infty\) gains
  - 6.2. `generateCF`: Generate Complementary Filters
    - Function description
    - Optional Parameters
    - H-Infinity Synthesis

In this document, the design of complementary filters is studied.

One use of complementary filter is described below:

> The basic idea of a complementary filter involves taking two or more sensors, filtering out unreliable frequencies for each sensor, and combining the filtered outputs to get a better estimate throughout the entire bandwidth of the system. To achieve this, the sensors included in the filter should complement one another by performing better over specific parts of the system bandwidth.

This document is divided into several sections:

- in section 1, the \(\mathcal{H}_\infty\) synthesis is used for generating two complementary filters
- in section 2, a method using the \(\mathcal{H}_\infty\) synthesis is proposed to shape three of more complementary filters
- in section 3, the \(\mathcal{H}_\infty\) synthesis is used and compared with FIR complementary filters used for LIGO

Add the Matlab code use to obtain the results presented in the paper are accessible here and presented below.

## 1 H-Infinity synthesis of complementary filters

The Matlab file corresponding to this section is accessible here.

### 1.1 Synthesis Architecture

We here synthesize two complementary filters using the \(\mathcal{H}_\infty\) synthesis. The goal is to specify upper bounds on the norms of the two complementary filters \(H_1(s)\) and \(H_2(s)\) while ensuring their complementary property (\(H_1(s) + H_2(s) = 1\)).

In order to do so, we use the generalized plant shown on figure 1 where \(W_1(s)\) and \(W_2(s)\) are weighting transfer functions that will be used to shape \(H_1(s)\) and \(H_2(s)\) respectively.

Figure 1: \(\mathcal{H}_\infty\) synthesis of the complementary filters

The \(\mathcal{H}_\infty\) synthesis applied on this generalized plant will give a transfer function \(H_2\) (figure 1) such that the \(\mathcal{H}_\infty\) norm of the transfer function from \(w\) to \([z_1,\ z_2]\) is less than one: \[ \left\| \begin{array}{c} (1 - H_2(s)) W_1(s) \\ H_2(s) W_2(s) \end{array} \right\|_\infty < 1 \]

Thus, if the above condition is verified, we can define \(H_1(s) = 1 - H_2(s)\) and we have that: \[ \left\| \begin{array}{c} H_1(s) W_1(s) \\ H_2(s) W_2(s) \end{array} \right\|_\infty < 1 \] Which is almost (with an maximum error of \(\sqrt{2}\)) equivalent to:

\begin{align*} |H_1(j\omega)| &< \frac{1}{|W_1(j\omega)|}, \quad \forall \omega \\ |H_2(j\omega)| &< \frac{1}{|W_2(j\omega)|}, \quad \forall \omega \end{align*}

We then see that \(W_1(s)\) and \(W_2(s)\) can be used to shape both \(H_1(s)\) and \(H_2(s)\) while ensuring their complementary property by the definition of \(H_1(s) = 1 - H_2(s)\).

### 1.2 Design of Weighting Function

A formula is proposed to help the design of the weighting functions:

\begin{equation} W(s) = \left( \frac{ \frac{1}{\omega_0} \sqrt{\frac{1 - \left(\frac{G_0}{G_c}\right)^{\frac{2}{n}}}{1 - \left(\frac{G_c}{G_\infty}\right)^{\frac{2}{n}}}} s + \left(\frac{G_0}{G_c}\right)^{\frac{1}{n}} }{ \left(\frac{1}{G_\infty}\right)^{\frac{1}{n}} \frac{1}{\omega_0} \sqrt{\frac{1 - \left(\frac{G_0}{G_c}\right)^{\frac{2}{n}}}{1 - \left(\frac{G_c}{G_\infty}\right)^{\frac{2}{n}}}} s + \left(\frac{1}{G_c}\right)^{\frac{1}{n}} }\right)^n \end{equation}

The parameters permits to specify:

- the low frequency gain: \(G_0 = lim_{\omega \to 0} |W(j\omega)|\)
- the high frequency gain: \(G_\infty = lim_{\omega \to \infty} |W(j\omega)|\)
- the absolute gain at \(\omega_0\): \(G_c = |W(j\omega_0)|\)
- the absolute slope between high and low frequency: \(n\)

The general shape of a weighting function generated using the formula is shown in figure 2.

Figure 2: Gain of the Weighting Function formula

    n = 2; w0 = 2*pi*11; G0 = 1/10; G1 = 1000; Gc = 1/2;
    W1 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

    n = 3; w0 = 2*pi*10; G0 = 1000; G1 = 0.1; Gc = 1/2;
    W2 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

Figure 3: Weights on the complementary filters \(W_1\) and \(W_2\) and the associated performance weights

### 1.3 H-Infinity Synthesis

We define the generalized plant \(P\) on matlab.

    P = [W1 -W1;
         0   W2;
         1   0];

And we do the \(\mathcal{H}_\infty\) synthesis using the `hinfsyn` command.

    [H2, ~, gamma, ~] = hinfsyn(P, 1, 1,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');

    [H2, ~, gamma, ~] = hinfsyn(P, 1, 1,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');
    Resetting value of Gamma min based on D_11, D_12, D_21 terms

    Test bounds:      0.1000 <  gamma  <=   1050.0000

      gamma    hamx_eig  xinf_eig  hamy_eig   yinf_eig   nrho_xy   p/f
    1.050e+03   2.8e+01   2.4e-07   4.1e+00    0.0e+00    0.0000    p
      525.050   2.8e+01   2.4e-07   4.1e+00    0.0e+00    0.0000    p
      262.575   2.8e+01   2.4e-07   4.1e+00    0.0e+00    0.0000    p
      131.337   2.8e+01   2.4e-07   4.1e+00   -1.0e-13    0.0000    p
       65.719   2.8e+01   2.4e-07   4.1e+00   -9.5e-14    0.0000    p
       32.909   2.8e+01   2.4e-07   4.1e+00    0.0e+00    0.0000    p
       16.505   2.8e+01   2.4e-07   4.1e+00   -1.0e-13    0.0000    p
        8.302   2.8e+01   2.4e-07   4.1e+00   -7.2e-14    0.0000    p
        4.201   2.8e+01   2.4e-07   4.1e+00   -2.5e-25    0.0000    p
        2.151   2.7e+01   2.4e-07   4.1e+00   -3.8e-14    0.0000    p
        1.125   2.6e+01   2.4e-07   4.1e+00   -5.4e-24    0.0000    p
        0.613   2.3e+01 -3.7e+01#  4.1e+00    0.0e+00    0.0000    f
        0.869   2.6e+01 -3.7e+02#  4.1e+00    0.0e+00    0.0000    f
        0.997   2.6e+01 -1.1e+04#  4.1e+00    0.0e+00    0.0000    f
        1.061   2.6e+01   2.4e-07   4.1e+00    0.0e+00    0.0000    p
        1.029   2.6e+01   2.4e-07   4.1e+00    0.0e+00    0.0000    p
        1.013   2.6e+01   2.4e-07   4.1e+00    0.0e+00    0.0000    p
        1.005   2.6e+01   2.4e-07   4.1e+00    0.0e+00    0.0000    p
        1.001   2.6e+01 -3.1e+04#  4.1e+00   -3.8e-14    0.0000    f
        1.003   2.6e+01 -2.8e+05#  4.1e+00    0.0e+00    0.0000    f
        1.004   2.6e+01   2.4e-07   4.1e+00   -5.8e-24    0.0000    p
        1.004   2.6e+01   2.4e-07   4.1e+00    0.0e+00    0.0000    p

     Gamma value achieved:     1.0036

We then define the high pass filter \(H_1 = 1 - H_2\). The bode plot of both \(H_1\) and \(H_2\) is shown on figure 4.

    H1 = 1 - H2;

### 1.4 Obtained Complementary Filters

The obtained complementary filters are shown on figure 4.

Figure 4: Obtained complementary filters using \(\mathcal{H}_\infty\) synthesis

## 2 Generating 3 complementary filters

The Matlab file corresponding to this section is accessible here.

### 2.1 Theory

We want:

\begin{align*} & |H_1(j\omega)| < 1/|W_1(j\omega)|, \quad \forall\omega\\ & |H_2(j\omega)| < 1/|W_2(j\omega)|, \quad \forall\omega\\ & |H_3(j\omega)| < 1/|W_3(j\omega)|, \quad \forall\omega\\ & H_1(s) + H_2(s) + H_3(s) = 1 \end{align*}

For that, we use the \(\mathcal{H}_\infty\) synthesis with the architecture shown on figure 5.

Figure 5: Generalized architecture for generating 3 complementary filters

The \(\mathcal{H}_\infty\) objective is:

\begin{align*} & |(1 - H_2(j\omega) - H_3(j\omega)) W_1(j\omega)| < 1, \quad \forall\omega\\ & |H_2(j\omega) W_2(j\omega)| < 1, \quad \forall\omega\\ & |H_3(j\omega) W_3(j\omega)| < 1, \quad \forall\omega\\ \end{align*}

And thus if we choose \(H_1 = 1 - H_2 - H_3\) we have solved the problem.

### 2.2 Weights

First we define the weights.

    n = 2; w0 = 2*pi*1; G0 = 1/10; G1 = 1000; Gc = 1/2;
    W1 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

    W2 = 0.22*(1 + s/2/pi/1)^2/(sqrt(1e-4) + s/2/pi/1)^2*(1 + s/2/pi/10)^2/(1 + s/2/pi/1000)^2;

    n = 3; w0 = 2*pi*10; G0 = 1000; G1 = 0.1; Gc = 1/2;
    W3 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

Figure 6: Three weighting functions used for the \(\mathcal{H}_\infty\) synthesis of the complementary filters

### 2.3 H-Infinity Synthesis

Then we create the generalized plant `P`.

    P = [W1 -W1 -W1;
         0   W2  0 ;
         0   0   W3;
         1   0   0];

And we do the \(\mathcal{H}_\infty\) synthesis.

    [H, ~, gamma, ~] = hinfsyn(P, 1, 2,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');

    [H, ~, gamma, ~] = hinfsyn(P, 1, 2,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');
    Resetting value of Gamma min based on D_11, D_12, D_21 terms

    Test bounds:      0.1000 <  gamma  <=   1050.0000

      gamma    hamx_eig  xinf_eig  hamy_eig   yinf_eig   nrho_xy   p/f
    1.050e+03   3.2e+00   4.5e-13   6.3e-02   -1.2e-11    0.0000    p
      525.050   3.2e+00   1.3e-13   6.3e-02    0.0e+00    0.0000    p
      262.575   3.2e+00   2.1e-12   6.3e-02   -1.5e-13    0.0000    p
      131.337   3.2e+00   1.1e-12   6.3e-02   -7.2e-29    0.0000    p
       65.719   3.2e+00   2.0e-12   6.3e-02    0.0e+00    0.0000    p
       32.909   3.2e+00   7.4e-13   6.3e-02   -5.9e-13    0.0000    p
       16.505   3.2e+00   1.4e-12   6.3e-02    0.0e+00    0.0000    p
        8.302   3.2e+00   1.6e-12   6.3e-02    0.0e+00    0.0000    p
        4.201   3.2e+00   1.6e-12   6.3e-02    0.0e+00    0.0000    p
        2.151   3.2e+00   1.6e-12   6.3e-02    0.0e+00    0.0000    p
        1.125   3.2e+00   2.8e-12   6.3e-02    0.0e+00    0.0000    p
        0.613   3.0e+00 -2.5e+03#  6.3e-02    0.0e+00    0.0000    f
        0.869   3.1e+00 -2.9e+01#  6.3e-02    0.0e+00    0.0000    f
        0.997   3.2e+00   1.9e-12   6.3e-02    0.0e+00    0.0000    p
        0.933   3.1e+00 -6.9e+02#  6.3e-02    0.0e+00    0.0000    f
        0.965   3.1e+00 -3.0e+03#  6.3e-02    0.0e+00    0.0000    f
        0.981   3.1e+00 -8.6e+03#  6.3e-02    0.0e+00    0.0000    f
        0.989   3.2e+00 -2.7e+04#  6.3e-02    0.0e+00    0.0000    f
        0.993   3.2e+00 -5.7e+05#  6.3e-02    0.0e+00    0.0000    f
        0.995   3.2e+00   2.2e-12   6.3e-02    0.0e+00    0.0000    p
        0.994   3.2e+00   1.6e-12   6.3e-02    0.0e+00    0.0000    p
        0.994   3.2e+00   1.0e-12   6.3e-02    0.0e+00    0.0000    p

     Gamma value achieved:     0.9936

### 2.4 Obtained Complementary Filters

The obtained filters are:

    H2 = tf(H(1));
    H3 = tf(H(2));
    H1 = 1 - H2 - H3;

Figure 7: The three complementary filters obtained after \(\mathcal{H}_\infty\) synthesis

## 3 Implement complementary filters for LIGO

The Matlab file corresponding to this section is accessible here.

Let’s try to design complementary filters that are corresponding to the complementary filters design for the LIGO and described in (Hua 2005).

The FIR complementary filters designed in (Hua 2005) are of order 512.

### 3.1 Specifications

The specifications for the filters are:

1. From \(0\) to \(0.008\text{ Hz}\),the magnitude of the filter’s transfer function should be less than or equal to \(8 \times 10^{-3}\)
2. From \(0.008\text{ Hz}\) to \(0.04\text{ Hz}\), it attenuates the input signal proportional to frequency cubed
3. Between \(0.04\text{ Hz}\) and \(0.1\text{ Hz}\), the magnitude of the transfer function should be less than 3
4. Above \(0.1\text{ Hz}\), the maximum of the magnitude of the complement filter should be as close to zero as possible. In our system, we would like to have the magnitude of the complementary filter to be less than \(0.1\). As the filters obtained in (Hua 2005) have a magnitude of \(0.045\), we will set that as our requirement

The specifications are translated in upper bounds of the complementary filters are shown on figure 8.

Figure 8: Specification for the LIGO complementary filters

### 3.2 FIR Filter

We here try to implement the FIR complementary filter synthesis as explained in (Hua 2005). For that, we use the CVX matlab Toolbox.

We setup the CVX toolbox and use the `SeDuMi` solver.

    cvx_startup;
    cvx_solver sedumi;

We define the frequency vectors on which we will constrain the norm of the FIR filter.

    w1 = 0:4.06e-4:0.008;
    w2 = 0.008:4.06e-4:0.04;
    w3 = 0.04:8.12e-4:0.1;
    w4 = 0.1:8.12e-4:0.83;

We then define the order of the FIR filter.

    n = 512;

    A1 = [ones(length(w1),1),  cos(kron(w1'.*(2*pi),[1:n-1]))];
    A2 = [ones(length(w2),1),  cos(kron(w2'.*(2*pi),[1:n-1]))];
    A3 = [ones(length(w3),1),  cos(kron(w3'.*(2*pi),[1:n-1]))];
    A4 = [ones(length(w4),1),  cos(kron(w4'.*(2*pi),[1:n-1]))];

    B1 = [zeros(length(w1),1), sin(kron(w1'.*(2*pi),[1:n-1]))];
    B2 = [zeros(length(w2),1), sin(kron(w2'.*(2*pi),[1:n-1]))];
    B3 = [zeros(length(w3),1), sin(kron(w3'.*(2*pi),[1:n-1]))];
    B4 = [zeros(length(w4),1), sin(kron(w4'.*(2*pi),[1:n-1]))];

We run the convex optimization.

    cvx_begin

    variable y(n+1,1)

    % t
    maximize(-y(1))

    for i = 1:length(w1)
        norm([0 A1(i,:); 0 B1(i,:)]*y) <= 8e-3;
    end

    for  i = 1:length(w2)
        norm([0 A2(i,:); 0 B2(i,:)]*y) <= 8e-3*(2*pi*w2(i)/(0.008*2*pi))^3;
    end

    for i = 1:length(w3)
        norm([0 A3(i,:); 0 B3(i,:)]*y) <= 3;
    end

    for i = 1:length(w4)
        norm([[1 0]'- [0 A4(i,:); 0 B4(i,:)]*y]) <= y(1);
    end

    cvx_end

    h = y(2:end);

    cvx_begin
    variable y(n+1,1)
    % t
    maximize(-y(1))
    for i = 1:length(w1)
        norm([0 A1(i,:); 0 B1(i,:)]*y) <= 8e-3;
    end
    for  i = 1:length(w2)
        norm([0 A2(i,:); 0 B2(i,:)]*y) <= 8e-3*(2*pi*w2(i)/(0.008*2*pi))^3;
    end
    for i = 1:length(w3)
        norm([0 A3(i,:); 0 B3(i,:)]*y) <= 3;
    end
    for i = 1:length(w4)
        norm([[1 0]'- [0 A4(i,:); 0 B4(i,:)]*y]) <= y(1);
    end
    cvx_end

    Calling SeDuMi 1.34: 4291 variables, 1586 equality constraints
       For improved efficiency, SeDuMi is solving the dual problem.
    ------------------------------------------------------------
    SeDuMi 1.34 (beta) by AdvOL, 2005-2008 and Jos F. Sturm, 1998-2003.
    Alg = 2: xz-corrector, Adaptive Step-Differentiation, theta = 0.250, beta = 0.500
    eqs m = 1586, order n = 3220, dim = 4292, blocks = 1073
    nnz(A) = 1100727 + 0, nnz(ADA) = 1364794, nnz(L) = 683190
     it :     b*y       gap    delta  rate   t/tP*  t/tD*   feas cg cg  prec
      0 :            4.11E+02 0.000
      1 :  -2.58E+00 1.25E+02 0.000 0.3049 0.9000 0.9000   4.87  1  1  3.0E+02
      2 :  -2.36E+00 3.90E+01 0.000 0.3118 0.9000 0.9000   1.83  1  1  6.6E+01
      3 :  -1.69E+00 1.31E+01 0.000 0.3354 0.9000 0.9000   1.76  1  1  1.5E+01
      4 :  -8.60E-01 7.10E+00 0.000 0.5424 0.9000 0.9000   2.48  1  1  4.8E+00
      5 :  -4.91E-01 5.44E+00 0.000 0.7661 0.9000 0.9000   3.12  1  1  2.5E+00
      6 :  -2.96E-01 3.88E+00 0.000 0.7140 0.9000 0.9000   2.62  1  1  1.4E+00
      7 :  -1.98E-01 2.82E+00 0.000 0.7271 0.9000 0.9000   2.14  1  1  8.5E-01
      8 :  -1.39E-01 2.00E+00 0.000 0.7092 0.9000 0.9000   1.78  1  1  5.4E-01
      9 :  -9.99E-02 1.30E+00 0.000 0.6494 0.9000 0.9000   1.51  1  1  3.3E-01
     10 :  -7.57E-02 8.03E-01 0.000 0.6175 0.9000 0.9000   1.31  1  1  2.0E-01
     11 :  -5.99E-02 4.22E-01 0.000 0.5257 0.9000 0.9000   1.17  1  1  1.0E-01
     12 :  -5.28E-02 2.45E-01 0.000 0.5808 0.9000 0.9000   1.08  1  1  5.9E-02
     13 :  -4.82E-02 1.28E-01 0.000 0.5218 0.9000 0.9000   1.05  1  1  3.1E-02
     14 :  -4.56E-02 5.65E-02 0.000 0.4417 0.9045 0.9000   1.02  1  1  1.4E-02
     15 :  -4.43E-02 2.41E-02 0.000 0.4265 0.9004 0.9000   1.01  1  1  6.0E-03
     16 :  -4.37E-02 8.90E-03 0.000 0.3690 0.9070 0.9000   1.00  1  1  2.3E-03
     17 :  -4.35E-02 3.24E-03 0.000 0.3641 0.9164 0.9000   1.00  1  1  9.5E-04
     18 :  -4.34E-02 1.55E-03 0.000 0.4788 0.9086 0.9000   1.00  1  1  4.7E-04
     19 :  -4.34E-02 8.77E-04 0.000 0.5653 0.9169 0.9000   1.00  1  1  2.8E-04
     20 :  -4.34E-02 5.05E-04 0.000 0.5754 0.9034 0.9000   1.00  1  1  1.6E-04
     21 :  -4.34E-02 2.94E-04 0.000 0.5829 0.9136 0.9000   1.00  1  1  9.9E-05
     22 :  -4.34E-02 1.63E-04 0.015 0.5548 0.9000 0.0000   1.00  1  1  6.6E-05
     23 :  -4.33E-02 9.42E-05 0.000 0.5774 0.9053 0.9000   1.00  1  1  3.9E-05
     24 :  -4.33E-02 6.27E-05 0.000 0.6658 0.9148 0.9000   1.00  1  1  2.6E-05
     25 :  -4.33E-02 3.75E-05 0.000 0.5972 0.9187 0.9000   1.00  1  1  1.6E-05
     26 :  -4.33E-02 1.89E-05 0.000 0.5041 0.9117 0.9000   1.00  1  1  8.6E-06
     27 :  -4.33E-02 9.72E-06 0.000 0.5149 0.9050 0.9000   1.00  1  1  4.5E-06
     28 :  -4.33E-02 2.94E-06 0.000 0.3021 0.9194 0.9000   1.00  1  1  1.5E-06
     29 :  -4.33E-02 9.73E-07 0.000 0.3312 0.9189 0.9000   1.00  2  2  5.3E-07
     30 :  -4.33E-02 2.82E-07 0.000 0.2895 0.9063 0.9000   1.00  2  2  1.6E-07
     31 :  -4.33E-02 8.05E-08 0.000 0.2859 0.9049 0.9000   1.00  2  2  4.7E-08
     32 :  -4.33E-02 1.43E-08 0.000 0.1772 0.9059 0.9000   1.00  2  2  8.8E-09

    iter seconds digits       c*x               b*y
     32     49.4   6.8 -4.3334083581e-02 -4.3334090214e-02
    |Ax-b| =   3.7e-09, [Ay-c]_+ =   1.1E-10, |x|=  1.0e+00, |y|=  2.6e+00

    Detailed timing (sec)
       Pre          IPM          Post
    3.902E+00    4.576E+01    1.035E-02
    Max-norms: ||b||=1, ||c|| = 3,
    Cholesky |add|=0, |skip| = 0, ||L.L|| = 4.26267.
    ------------------------------------------------------------
    Status: Solved
    Optimal value (cvx_optval): -0.0433341
    h = y(2:end);

Finally, we compute the filter response over the frequency vector defined and the result is shown on figure 9 which is very close to the filters obtain in (Hua 2005).

    w = [w1 w2 w3 w4];
    H = [exp(-j*kron(w'.*2*pi,[0:n-1]))]*h;

Figure 9: FIR Complementary filters obtain after convex optimization

### 3.3 Weights

We design weights that will be used for the \(\mathcal{H}_\infty\) synthesis of the complementary filters. These weights will determine the order of the obtained filters. Here are the requirements on the filters:

- reasonable order
- to be as close as possible to the specified upper bounds
- stable minimum phase

The bode plot of the weights is shown on figure 10.

Figure 10: Weights for the \(\mathcal{H}_\infty\) synthesis

### 3.4 H-Infinity Synthesis

We define the generalized plant as shown on figure 1.

    P = [0   wL;
         wH -wH;
         1   0];

And we do the \(\mathcal{H}_\infty\) synthesis using the `hinfsyn` command.

    [Hl, ~, gamma, ~] = hinfsyn(P, 1, 1,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');

    [Hl, ~, gamma, ~] = hinfsyn(P, 1, 1,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');
    Resetting value of Gamma min based on D_11, D_12, D_21 terms

    Test bounds:      0.3276 <  gamma  <=      1.8063

      gamma    hamx_eig  xinf_eig  hamy_eig   yinf_eig   nrho_xy   p/f
        1.806   1.4e-02 -1.7e-16   3.6e-03   -4.8e-12    0.0000    p
        1.067   1.3e-02 -4.2e-14   3.6e-03   -1.9e-12    0.0000    p
        0.697   1.3e-02 -3.0e-01#  3.6e-03   -3.5e-11    0.0000    f
        0.882   1.3e-02 -9.5e-01#  3.6e-03   -1.2e-34    0.0000    f
        0.975   1.3e-02 -2.7e+00#  3.6e-03   -1.6e-12    0.0000    f
        1.021   1.3e-02 -8.7e+00#  3.6e-03   -4.5e-16    0.0000    f
        1.044   1.3e-02 -6.5e-14   3.6e-03   -3.0e-15    0.0000    p
        1.032   1.3e-02 -1.8e+01#  3.6e-03    0.0e+00    0.0000    f
        1.038   1.3e-02 -3.8e+01#  3.6e-03    0.0e+00    0.0000    f
        1.041   1.3e-02 -8.3e+01#  3.6e-03   -2.9e-33    0.0000    f
        1.042   1.3e-02 -1.9e+02#  3.6e-03   -3.4e-11    0.0000    f
        1.043   1.3e-02 -5.3e+02#  3.6e-03   -7.5e-13    0.0000    f

     Gamma value achieved:     1.0439

The high pass filter is defined as \(H_H = 1 - H_L\).

    Hh = 1 - Hl;

The size of the filters is shown below.

    size(Hh), size(Hl)
    State-space model with 1 outputs, 1 inputs, and 27 states.
    State-space model with 1 outputs, 1 inputs, and 27 states.

The bode plot of the obtained filters as shown on figure 11.

Figure 11: Obtained complementary filters using the \(\mathcal{H}_\infty\) synthesis

### 3.5 Compare FIR and H-Infinity Filters

Let’s now compare the FIR filters designed in (Hua 2005) and the one obtained with the \(\mathcal{H}_\infty\) synthesis on figure 12.

Figure 12: Comparison between the FIR filters developped for LIGO and the \(\mathcal{H}_\infty\) complementary filters

## 4 Alternative Synthesis

### 4.1 Two generalized plants

In order to synthesize the complementary filter using the proposed method, we can use two alternative generalized plant as shown in Figures 13 and 14.

\begin{equation} P_1 = \begin{bmatrix} W_1 & -W_1 \\ 0 & W_2 \\ 1 & 0 \end{bmatrix} \end{equation}

Figure 13: Complementary Filter Synthesis - Conf 1

\begin{equation} P_2 = \begin{bmatrix} 0 & W_1 & 1 \\ W_2 & -W_1 & 0 \end{bmatrix} \end{equation}

Figure 14: Complementary Filter Synthesis - Conf 2

Let’s run the \(\mathcal{H}_\infty\) synthesis for both generalized plant using the same weights and see if the obtained filters are the same:

    n = 2; w0 = 2*pi*11; G0 = 1/10; G1 = 1000; Gc = 1/2;
    W1 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

    n = 3; w0 = 2*pi*10; G0 = 1000; G1 = 0.1; Gc = 1/2;
    W2 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

    P1 = [W1 -W1;
          0   W2;
          1   0];

    [H2, ~, gamma, ~] = hinfsyn(P1, 1, 1,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');

    [H2, ~, gamma, ~] = hinfsyn(P1, 1, 1,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');

      Test bounds:  0.3263 <=  gamma  <=  1000

        gamma        X>=0        Y>=0       rho(XY)<1    p/f
      1.807e+01     1.4e-07     0.0e+00     1.185e-18     p
      2.428e+00     1.5e-07     0.0e+00     1.285e-18     p
      8.902e-01    -2.9e+02 #  -7.1e-17     5.168e-19     f
      1.470e+00     1.5e-07     0.0e+00     1.462e-14     p
      1.144e+00     1.5e-07     0.0e+00     1.260e-14     p
      1.009e+00     1.5e-07     0.0e+00     4.120e-13     p
      9.478e-01    -6.8e+02 #  -2.4e-17     1.449e-14     f
      9.780e-01    -1.6e+03 #  -7.3e-17     6.791e-14     f
      9.934e-01    -4.2e+03 #  -1.2e-16     3.524e-14     f
      1.001e+00    -2.0e+04 #  -2.3e-17     5.717e-20     f
      1.005e+00     1.5e-07     0.0e+00     8.953e-18     p
      1.003e+00    -2.2e+05 #  -1.8e-17     3.225e-12     f
      1.004e+00     1.5e-07     0.0e+00     2.445e-12     p
      Limiting gains...
      1.004e+00     1.6e-07     0.0e+00     5.811e-18     p

      Best performance (actual): 1.004

    P2 = [0   W1 1;
          W2 -W1 0];

    [H2b, ~, gamma, ~] = hinfsyn(P2, 1, 1,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');

    [H2b, ~, gamma, ~] = hinfsyn(P2, 1, 1,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');

      Test bounds:  0.3263 <=  gamma  <=  1000

        gamma        X>=0        Y>=0       rho(XY)<1    p/f
      1.807e+01     0.0e+00     1.4e-07     2.055e-16     p
      2.428e+00     0.0e+00     1.4e-07     1.894e-18     p
      8.902e-01    -2.1e-16    -2.7e+02 #   1.466e-16     f
      1.470e+00     0.0e+00     1.4e-07     4.118e-16     p
      1.144e+00     0.0e+00     1.5e-07     2.105e-18     p
      1.009e+00     0.0e+00     1.5e-07     2.590e-13     p
      9.478e-01    -9.5e-17    -6.3e+02 #   1.663e-19     f
      9.780e-01    -1.1e-16    -1.5e+03 #   1.546e-14     f
      9.934e-01    -2.8e-17    -4.0e+03 #   3.934e-14     f
      1.001e+00    -3.1e-17    -1.9e+04 #   1.191e-19     f
      1.005e+00     0.0e+00     1.5e-07     1.443e-12     p
      1.003e+00    -8.3e-17    -2.1e+05 #   8.807e-13     f
      1.004e+00     0.0e+00     1.5e-07     1.459e-15     p
      Limiting gains...
      1.004e+00     0.0e+00     1.5e-07     9.086e-19     p

      Best performance (actual): 1.004

And indeed, we can see that the exact same filters are obtained (Figure 15).

Figure 15: Comparison of \(H_2(s)\) when using \(P_1(s)\) or \(P_2(s)\)

### 4.2 Shaping the Low pass filter or the high pass filter?

Let’s see if there is a difference by explicitly shaping \(H_1(s)\) or \(H_2(s)\).

    n = 2; w0 = 2*pi*11; G0 = 1/10; G1 = 1000; Gc = 1/2;
    W1 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

    n = 3; w0 = 2*pi*10; G0 = 1000; G1 = 0.1; Gc = 1/2;
    W2 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

Let’s first synthesize \(H_1(s)\):

    P1 = [W2 -W2;
          0   W1;
          1   0];

    [H1, ~, gamma, ~] = hinfsyn(P1, 1, 1,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');

    [H1, ~, gamma, ~] = hinfsyn(P1, 1, 1,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');

      Test bounds:  0.3263 <=  gamma  <=  1.712

        gamma        X>=0        Y>=0       rho(XY)<1    p/f
      7.476e-01    -2.5e+01 #  -8.3e-18     4.938e-20     f
      1.131e+00     1.9e-07     0.0e+00     1.566e-16     p
      9.197e-01    -1.4e+02 #  -7.9e-17     4.241e-17     f
      1.020e+00     1.9e-07     0.0e+00     2.095e-16     p
      9.686e-01    -3.8e+02 #  -7.0e-17     1.463e-23     f
      9.940e-01    -1.5e+03 #  -1.3e-17     3.168e-19     f
      1.007e+00     1.9e-07     0.0e+00     1.696e-15     p
      1.000e+00    -4.8e+03 #  -7.1e-18     7.203e-20     f
      1.004e+00     1.9e-07     0.0e+00     1.491e-14     p
      1.002e+00    -1.1e+04 #  -2.6e-16     2.579e-14     f
      1.003e+00    -2.8e+04 #  -6.0e-18     8.558e-20     f
      Limiting gains...
      1.004e+00     2.0e-07     0.0e+00     5.647e-18     p
      1.004e+00     1.0e-06     0.0e+00     5.648e-18     p

      Best performance (actual): 1.004

And now \(H_2(s)\):

    P2 = [W1 -W1;
          0   W2;
          1   0];

    [H2, ~, gamma, ~] = hinfsyn(P2, 1, 1,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');

    [H2b, ~, gamma, ~] = hinfsyn(P2, 1, 1,'TOLGAM', 0.001, 'METHOD', 'ric', 'DISPLAY', 'on');

      Test bounds:  0.3263 <=  gamma  <=  1000

        gamma        X>=0        Y>=0       rho(XY)<1    p/f
      1.807e+01     1.4e-07     0.0e+00     1.185e-18     p
      2.428e+00     1.5e-07     0.0e+00     1.285e-18     p
      8.902e-01    -2.9e+02 #  -7.1e-17     5.168e-19     f
      1.470e+00     1.5e-07     0.0e+00     1.462e-14     p
      1.144e+00     1.5e-07     0.0e+00     1.260e-14     p
      1.009e+00     1.5e-07     0.0e+00     4.120e-13     p
      9.478e-01    -6.8e+02 #  -2.4e-17     1.449e-14     f
      9.780e-01    -1.6e+03 #  -7.3e-17     6.791e-14     f
      9.934e-01    -4.2e+03 #  -1.2e-16     3.524e-14     f
      1.001e+00    -2.0e+04 #  -2.3e-17     5.717e-20     f
      1.005e+00     1.5e-07     0.0e+00     8.953e-18     p
      1.003e+00    -2.2e+05 #  -1.8e-17     3.225e-12     f
      1.004e+00     1.5e-07     0.0e+00     2.445e-12     p
      Limiting gains...
      1.004e+00     1.6e-07     0.0e+00     5.811e-18     p

      Best performance (actual): 1.004

And compare \(H_1(s)\) with \(1 - H_2(s)\) and \(H_2(s)\) with \(1 - H_1(s)\) in Figure 16.

Figure 16: Comparison of \(H_1(s)\) with \(1-H_2(s)\), and \(H_2(s)\) with \(1-H_1(s)\)

### 4.3 Using Feedback architecture

    n = 2; w0 = 2*pi*11; G0 = 1/10; G1 = 1000; Gc = 1/2;
    W1 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

    n = 3; w0 = 2*pi*10; G0 = 1000; G1 = 0.1; Gc = 1/2;
    W2 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

Let’s first synthesize \(H_1(s)\):

    P = [W1 -W1;
         0   W2;
         1  -1];

    [K, ~, gamma, ~] = hinfsyn(P, 1, 1,'TOLGAM', 0.001, 'METHOD', 'lmi', 'DISPLAY', 'on');

    H1 = inv(1 + K);
    H2 = 1 - H1;

### 4.4 Adding feature in the filters

    n = 2; w0 = 2*pi*11; G0 = 1/10; G1 = 1000; Gc = 1/2;
    W1 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

    n = 3; w0 = 2*pi*10; G0 = 1000; G1 = 0.1; Gc = 1/2;
    W2 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

    Wf = (1 + s/2/pi/1)/s;
    Wf = s/(1 + s/2/pi/1e2);

    % W2 = W2/Wf/(1 + s/2/pi/1e3);

    P = [W1 -Wf*W1;
         0   Wf*W2;
         1  -Wf];

    [Ka, ~, gamma, ~] = hinfsyn(P, 1, 1,'TOLGAM', 0.001, 'METHOD', 'lmi', 'DISPLAY', 'on');

    K = Ka*Wf;

    H1 = inv(1 + K);
    H2 = 1 - H1;

## 5 Impose a positive slope at DC or a negative slope at infinite frequency

### 5.1 Manually shift zeros to the origin after synthesis

Suppose we want \(H_2(s)\) to be an high pass filter with a slope of +2 at low frequency (from 0Hz).

We cannot impose that using the weight \(W_2(s)\) as it would be improper.

However, we may manually shift 2 of the low frequency zeros to the origin.

    n = 2; w0 = 2*pi*11; G0 = 1/10; G1 = 1000; Gc = 1/2;
    W1 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

    n = 3; w0 = 2*pi*10; G0 = 1e4; G1 = 0.1; Gc = 1/2;
    W2 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

    P = [W1 -W1;
         0   W2;
         1   0];

And we do the \(\mathcal{H}_\infty\) synthesis using the `hinfsyn` command:

    [H2, ~, gamma, ~] = hinfsyn(P, 1, 1,'TOLGAM', 0.001, 'METHOD', 'lmi', 'DISPLAY', 'on');

    [z,p,k] = zpkdata(H2)

Looking at the zeros, we see two low frequency complex conjugate zeros.

    z{1}
    ans =
              -4690930.24283199 +                     0i
              -163.420524657426 +                     0i
             -0.853192261081498 +     0.713416012479897i
             -0.853192261081498 -     0.713416012479897i
              -3.15812268762265 +                     0i

We manually put these zeros at the origin:

    z{1}([3,4]) = 0;

And we create a modified filter \(H_{2z}(s)\):

    H2z = zpk(z,p,k);

And as usual, \(H_{1z}(s)\) is defined as the complementary of \(H_{2z}(s)\):

    H1z = 1 - H2z;

The bode plots of \(H_1(s)\), \(H_2(s)\), \(H_{1z}(s)\) and \(H_{2z}(s)\) are shown in Figure 17. And we see that \(H_{1z}(s)\) is slightly modified when setting the zeros at the origin for \(H_{2z}(s)\).

Figure 17: Bode plots of \(H_1(s)\), \(H_2(s)\), \(H_{1z}(s)\) and \(H_{2z}(s)\)

### 5.2 Imposing a positive slope at DC during the synthesis phase

Suppose we want to synthesize \(H_2(s)\) such that it has a slope of +2 from DC. We can include this “feature” in the generalized plant as shown in Figure 18.

Figure 18: Generalized plant with included wanted feature represented by \(H_{2w}(s)\)

After synthesis, the obtained filter will be:

\begin{equation} H_2(s) = H_2^\prime(s) H_{2w}(s) \end{equation}

and therefore the “feature” will be included in the filter.

For \(H_1(s)\) nothing is changed: \(H_1(s) = 1 - H_2(s)\).

The weighting functions are defined as usual:

    n = 2; w0 = 2*pi*11; G0 = 1/10; G1 = 1000; Gc = 1/2;
    W1 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

    n = 3; w0 = 2*pi*10; G0 = 1e4; G1 = 0.1; Gc = 1/2;
    W2 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

The wanted feature here is a +2 slope at low frequency. For that, we use an high pass filter with a slope of +2 at low frequency.

    w0 = 2*pi*50;
    H2w = (s/w0/(s/w0+1))^2;

We define the generalized plant as shown in Figure 18.

    P = [W1 -W1;
         0   W2;
         H2w 0];

And we do the \(\mathcal{H}_\infty\) synthesis using the `hinfsyn` command.

    [H2p, ~, gamma, ~] = hinfsyn(P, 1, 1,'TOLGAM', 0.001, 'METHOD', 'lmi', 'DISPLAY', 'on');

Finally, we define \(H_2(s)\) as the product of the synthesized filter and the wanted “feature”:

    H2 = H2p*H2w;

And we define \(H_1(s)\) to be the complementary of \(H_2(s)\):

    H1 = 1 - H2;

The obtained complementary filters are shown in Figure 19.

Figure 19: Obtained complementary fitlers

### 5.3 Imposing a negative slope at infinity frequency during the synthesis phase

Let’s suppose we now want to shape a low pass filter that as a negative slope until infinite frequency.

The used technique is the same as in the previous section, and the generalized plant is shown in Figure 18.

The weights are defined as usual.

    n = 3; w0 = 2*pi*10; G0 = 1000; G1 = 0.1; Gc = 1/2;
    W1 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

    n = 2; w0 = 2*pi*11; G0 = 1/10; G1 = 1000; Gc = 1/2;
    W2 = (((1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (G0/Gc)^(1/n))/((1/G1)^(1/n)*(1/w0)*sqrt((1-(G0/Gc)^(2/n))/(1-(Gc/G1)^(2/n)))*s + (1/Gc)^(1/n)))^n;

This time, the feature is a low pass filter with a slope of -2 at high frequency.

    H2w = 1/(s/(2*pi*10) + 1)^2;

The generalized plant is defined:

    P = [W1 -W1;
         0   W2;
         H2w 0];

And we do the \(\mathcal{H}_\infty\) synthesis using the `hinfsyn` command.

    [H2p, ~, gamma, ~] = hinfsyn(P, 1, 1,'TOLGAM', 0.001, 'METHOD', 'lmi', 'DISPLAY', 'on');

The feature is added to the synthesized filter:

    H2 = H2p*H2w;

And \(H_1(s)\) is defined as follows:

    H1 = 1 - H2;

The obtained complementary filters are shown in Figure 20.

Figure 20: Obtained complementary fitlers

## Bibliography

Hua, Wensheng. 2005. “Low Frequency Vibration Isolation and Alignment System for Advanced LIGO.” stanford university.

## 6 Functions

### 6.1 `generateWF`: Generate Weighting Functions

This Matlab function is accessible here.

#### Function description

    function [W] = generateWF(args)
    % createWeight -
    %
    % Syntax: [W] = generateWeight(args)
    %
    % Inputs:
    %    - n  - Weight Order (integer)
    %    - G0 - Low frequency Gain
    %    - G1 - High frequency Gain
    %    - Gc - Gain of the weight at frequency w0
    %    - w0 - Frequency at which |W(j w0)| = Gc [rad/s]
    %
    % Outputs:
    %    - W - Generated Weight

#### Optional Parameters

    arguments
        args.n    (1,1) double {mustBeInteger, mustBePositive} = 1
        args.G0   (1,1) double {mustBeNumeric, mustBePositive} = 0.1
        args.Ginf (1,1) double {mustBeNumeric, mustBePositive} = 10
        args.Gc   (1,1) double {mustBeNumeric, mustBePositive} = 1
        args.w0   (1,1) double {mustBeNumeric, mustBePositive} = 1
    end

    mustBeBetween(args.G0, args.Gc, args.Ginf);

#### Generate the Weighting function

    s = zpk('s');

    W = (((1/args.w0)*sqrt((1-(args.G0/args.Gc)^(2/args.n))/(1-(args.Gc/args.Ginf)^(2/args.n)))*s + ...
          (args.G0/args.Gc)^(1/args.n))/...
         ((1/args.Ginf)^(1/args.n)*(1/args.w0)*sqrt((1-(args.G0/args.Gc)^(2/args.n))/(1-(args.Gc/args.Ginf)^(2/args.n)))*s + ...
          (1/args.Gc)^(1/args.n)))^args.n;

#### Verification of the \(G_0\), \(G_c\) and \(G_\infty\) gains

    % Custom validation function
    function mustBeBetween(a,b,c)
        if ~((a > b && b > c) || (c > b && b > a))
            eid = 'createWeight:inputError';
            msg = 'Gc should be between G0 and Ginf.';
            throwAsCaller(MException(eid,msg))
        end

### 6.2 `generateCF`: Generate Complementary Filters

This Matlab function is accessible here.

#### Function description

    function [H1, H2] = generateCF(W1, W2, args)
    % createWeight -
    %
    % Syntax: [W] = generateCF(args)
    %
    % Inputs:
    %    - W1 - Weighting Function for H1
    %    - W2 - Weighting Function for H2
    %    - args:
    %      - method  - H-Infinity solver ('lmi' or 'ric')
    %      - display - Display synthesis results ('on' or 'off')
    %
    % Outputs:
    %    - H1 - Generated H1 Filter
    %    - H2 - Generated H2 Filter

#### Optional Parameters

    arguments
        W1
        W2
        args.method  char {mustBeMember(args.method,{'lmi', 'ric'})} = 'ric'
        args.display char {mustBeMember(args.display,{'on', 'off'})} = 'on'
    end

#### H-Infinity Synthesis

    P = [W1 -W1;
         0   W2;
         1   0];

    [H2, ~, gamma, ~] = hinfsyn(P, 1, 1,'TOLGAM', 0.001, 'METHOD', args.method, 'DISPLAY', args.display);

    H1 = 1 - H2;

Author: Thomas Dehaeze

Created: 2021-04-29 jeu. 17:25