#+TITLE: Diagonal control using the SVD and the Jacobian Matrix
:DRAWER:
#+STARTUP: overview

#+LANGUAGE: en
#+EMAIL: dehaeze.thomas@gmail.com
#+AUTHOR: Dehaeze Thomas

#+HTML_LINK_HOME: ../index.html
#+HTML_LINK_UP:   ../index.html

#+HTML_HEAD: <link rel="stylesheet" type="text/css" href="https://research.tdehaeze.xyz/css/style.css"/>
#+HTML_HEAD: <script type="text/javascript" src="https://research.tdehaeze.xyz/js/script.js"></script>

#+LaTeX_CLASS: scrreprt
#+LaTeX_HEADER_EXTRA: \input{preamble.tex}

#+HTML_MATHJAX: align: center tagside: right font: TeX

#+PROPERTY: header-args:matlab  :session *MATLAB*
#+PROPERTY: header-args:matlab+ :comments org
#+PROPERTY: header-args:matlab+ :results none
#+PROPERTY: header-args:matlab+ :exports both
#+PROPERTY: header-args:matlab+ :eval no-export
#+PROPERTY: header-args:matlab+ :output-dir figs
#+PROPERTY: header-args:matlab+ :tangle no
#+PROPERTY: header-args:matlab+ :mkdirp yes

#+PROPERTY: header-args:shell  :eval no-export

#+PROPERTY: header-args:latex  :headers '("\\usepackage{tikz}" "\\usepackage{import}" "\\import{$HOME/Cloud/tikz/org/}{config.tex}")
#+PROPERTY: header-args:latex+ :imagemagick t :fit yes
#+PROPERTY: header-args:latex+ :iminoptions -scale 100% -density 150
#+PROPERTY: header-args:latex+ :imoutoptions -quality 100
#+PROPERTY: header-args:latex+ :results file raw replace
#+PROPERTY: header-args:latex+ :buffer no
#+PROPERTY: header-args:latex+ :eval no-export
#+PROPERTY: header-args:latex+ :exports results
#+PROPERTY: header-args:latex+ :mkdirp yes
#+PROPERTY: header-args:latex+ :output-dir figs
#+PROPERTY: header-args:latex+ :post pdf2svg(file=*this*, ext="png")
:END:

* Introduction                                                        :ignore:

In this document, the use of the Jacobian matrix and the Singular Value Decomposition to render a physical plant diagonal dominant is studied.
Then, a diagonal controller is used.

These two methods are tested on two plants:
- In Section [[sec:gravimeter]] on a 3-DoF gravimeter
- In Section [[sec:stewart_platform]] on a 6-DoF Stewart platform

* Gravimeter - Simscape Model
:PROPERTIES:
:header-args:matlab+: :tangle gravimeter/script.m
:END:
<<sec:gravimeter>>

** Introduction

In this part, diagonal control using both the SVD and the Jacobian matrices are applied on a gravimeter model:
- Section [[sec:gravimeter_model]]: the model is described and its parameters are defined.
- Section [[sec:gravimeter_identification]]: the plant dynamics from the actuators to the sensors is computed from a Simscape model.
- Section [[sec:gravimeter_jacobian_decoupling]]: the plant is decoupled using the Jacobian matrices.
- Section [[sec:gravimeter_svd_decoupling]]: the Singular Value Decomposition is performed on a real approximation of the plant transfer matrix and further use to decouple the system.
- Section [[sec:gravimeter_gershgorin_radii]]: the effectiveness of the decoupling is computed using the Gershorin radii
- Section [[sec:gravimeter_rga]]: the effectiveness of the decoupling is computed using the Relative Gain Array
- Section [[sec:gravimeter_decoupled_plant]]: the obtained decoupled plants are compared
- Section [[sec:gravimeter_diagonal_control]]: the diagonal controller is developed
- Section [[sec:gravimeter_closed_loop_results]]: the obtained closed-loop performances for the two methods are compared

** Matlab Init                                              :noexport:ignore:
#+begin_src matlab :tangle no :exports none :results silent :noweb yes :var current_dir=(file-name-directory buffer-file-name)
  <<matlab-dir>>
#+end_src

#+begin_src matlab :exports none :results silent :noweb yes
  <<matlab-init>>
#+end_src

#+begin_src matlab :tangle no
  addpath('gravimeter');
#+end_src

#+begin_src matlab
  freqs = logspace(-1, 2, 1000);
#+end_src

** Gravimeter Model - Parameters
<<sec:gravimeter_model>>

#+begin_src matlab :exports none
  open('gravimeter.slx')
#+end_src

The model of the gravimeter is schematically shown in Figure [[fig:gravimeter_model]].

#+name: fig:gravimeter_model
#+caption: Model of the gravimeter
[[file:figs/gravimeter_model.png]]

#+name: fig:leg_model
#+caption: Model of the struts
[[file:figs/leg_model.png]]

The parameters used for the simulation are the following:
#+begin_src matlab
  l  = 1.0; % Length of the mass [m]
  h  = 1.7; % Height of the mass [m]

  la = l/2; % Position of Act. [m]
  ha = h/2; % Position of Act. [m]

  m = 400; % Mass [kg]
  I = 115; % Inertia [kg m^2]

  k = 15e3; % Actuator Stiffness [N/m]
  c = 2e1; % Actuator Damping [N/(m/s)]

  deq = 0.2; % Length of the actuators [m]

  g = 0; % Gravity [m/s2]
#+end_src

** System Identification
<<sec:gravimeter_identification>>

#+begin_src matlab
  %% Name of the Simulink File
  mdl = 'gravimeter';

  %% Input/Output definition
  clear io; io_i = 1;
  io(io_i) = linio([mdl, '/F1'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/F2'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/F3'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_side'], 1, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_side'], 2, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_top'], 1, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_top'], 2, 'openoutput'); io_i = io_i + 1;

  G = linearize(mdl, io);
  G.InputName  = {'F1', 'F2', 'F3'};
  G.OutputName = {'Ax1', 'Ay1', 'Ax2', 'Ay2'};
#+end_src

The inputs and outputs of the plant are shown in Figure [[fig:gravimeter_plant_schematic]].

More precisely there are three inputs (the three actuator forces):
\begin{equation}
  \bm{\tau} = \begin{bmatrix}\tau_1 \\ \tau_2 \\ \tau_2 \end{bmatrix}
\end{equation}
And 4 outputs (the two 2-DoF accelerometers):
\begin{equation}
  \bm{a} = \begin{bmatrix} a_{1x} \\ a_{1y} \\ a_{2x} \\ a_{2y} \end{bmatrix}
\end{equation}

#+begin_src latex :file gravimeter_plant_schematic.pdf :tangle no :exports results
  \begin{tikzpicture}
    \node[block] (G) {$\bm{G}$};

    % Connections and labels
    \draw[<-] (G.west) -- ++(-2.0, 0) node[above right]{$\bm{\tau} = \begin{bmatrix}\tau_1 \\ \tau_2 \\ \tau_2 \end{bmatrix}$};
    \draw[->] (G.east) -- ++( 2.0, 0)  node[above left]{$\bm{a} = \begin{bmatrix} a_{1x} \\ a_{1y} \\ a_{2x} \\ a_{2y} \end{bmatrix}$};
  \end{tikzpicture}
#+end_src

#+name: fig:gravimeter_plant_schematic
#+caption: Schematic of the gravimeter plant
#+RESULTS:
[[file:figs/gravimeter_plant_schematic.png]]

We can check the poles of the plant:
#+begin_src matlab :results value replace :exports results
  pole(G)
#+end_src

#+RESULTS:
| -0.12243+13.551i   |
| -0.12243-13.551i   |
| -0.05+8.6601i      |
| -0.05-8.6601i      |
| -0.0088785+3.6493i |
| -0.0088785-3.6493i |

As expected, the plant as 6 states (2 translations + 1 rotation)
#+begin_src matlab :results output replace
  size(G)
#+end_src

#+RESULTS:
: State-space model with 4 outputs, 3 inputs, and 6 states.

The bode plot of all elements of the plant are shown in Figure [[fig:open_loop_tf]].

#+begin_src matlab :exports none
  figure;
  tiledlayout(4, 3, 'TileSpacing', 'None', 'Padding', 'None');

  for out_i = 1:4
      for in_i = 1:3
          nexttile;
          plot(freqs, abs(squeeze(freqresp(G(out_i,in_i), freqs, 'Hz'))), '-');
          set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
          xlim([1e-1, 2e1]); ylim([1e-4, 1e0]);

          if in_i == 1
              ylabel('Amplitude [m/N]')
          else
              set(gca, 'YTickLabel',[]);
          end

          if out_i == 4
              xlabel('Frequency [Hz]')
          else
              set(gca, 'XTickLabel',[]);
          end
      end
  end
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/open_loop_tf.pdf', 'width', 'full', 'height', 'full');
#+end_src

#+name: fig:open_loop_tf
#+attr_latex: :width \linewidth
#+caption: Open Loop Transfer Function from 3 Actuators to 4 Accelerometers
#+RESULTS:
[[file:figs/open_loop_tf.png]]

** Decoupling using the Jacobian
<<sec:gravimeter_jacobian_decoupling>>

Consider the control architecture shown in Figure [[fig:gravimeter_decouple_jacobian]].

The Jacobian matrix $J_{\tau}$ is used to transform forces applied by the three actuators into forces/torques applied on the gravimeter at its center of mass:
\begin{equation}
  \begin{bmatrix} \tau_1 \\ \tau_2 \\ \tau_3 \end{bmatrix} = J_{\tau}^{-T} \begin{bmatrix} F_x \\ F_y \\ M_z \end{bmatrix}
\end{equation}

The Jacobian matrix $J_{a}$ is used to compute the vertical acceleration, horizontal acceleration and rotational acceleration of the mass with respect to its center of mass:
\begin{equation}
  \begin{bmatrix} a_x \\ a_y \\ a_{R_z} \end{bmatrix} = J_{a}^{-1} \begin{bmatrix} a_{x1} \\ a_{y1} \\ a_{x2} \\ a_{y2} \end{bmatrix}
\end{equation}

We thus define a new plant as defined in Figure [[fig:gravimeter_decouple_jacobian]].
\[ \bm{G}_x(s) = J_a^{-1} \bm{G}(s) J_{\tau}^{-T} \]

$\bm{G}_x(s)$ correspond to the $3 \times 3$transfer function matrix from forces and torques applied to the gravimeter at its center of mass to the absolute acceleration of the gravimeter's center of mass (Figure [[fig:gravimeter_decouple_jacobian]]).

#+begin_src latex :file gravimeter_decouple_jacobian.pdf :tangle no :exports results
  \begin{tikzpicture}
    \node[block] (G) {$\bm{G}$};
    \node[block, left=0.6 of G] (Jt) {$J_{\tau}^{-T}$};
    \node[block, right=0.6 of G] (Ja) {$J_{a}^{-1}$};

    % Connections and labels
    \draw[<-] (Jt.west) -- ++(-2.5, 0) node[above right]{$\bm{\mathcal{F}} = \begin{bmatrix}F_x \\ F_y \\ M_z \end{bmatrix}$};
    \draw[->] (Jt.east) -- (G.west)  node[above left]{$\bm{\tau}$};
    \draw[->] (G.east) -- (Ja.west)  node[above left]{$\bm{a}$};
    \draw[->] (Ja.east) -- ++( 2.6, 0)  node[above left]{$\bm{\mathcal{A}} = \begin{bmatrix}a_x \\ a_y \\ a_{R_z} \end{bmatrix}$};

    \begin{scope}[on background layer]
      \node[fit={(Jt.south west) (Ja.north east)}, fill=black!10!white, draw, dashed, inner sep=14pt] (Gx) {};
      \node[below right] at (Gx.north west) {$\bm{G}_x$};
    \end{scope}
  \end{tikzpicture}
#+end_src

#+name: fig:gravimeter_decouple_jacobian
#+caption: Decoupled plant $\bm{G}_x$ using the Jacobian matrix $J$
#+RESULTS:
[[file:figs/gravimeter_decouple_jacobian.png]]

The Jacobian corresponding to the sensors and actuators are defined below:
#+begin_src matlab
  Ja = [1 0 -h/2
        0 1  l/2
        1 0  h/2
        0 1  0];

  Jt = [1 0 -ha
        0 1  la
        0 1 -la];
#+end_src

And the plant $\bm{G}_x$ is computed:
#+begin_src matlab
  Gx = pinv(Ja)*G*pinv(Jt');
  Gx.InputName  = {'Fx', 'Fy', 'Mz'};
  Gx.OutputName  = {'Dx', 'Dy', 'Rz'};
#+end_src

#+begin_src matlab :results output replace :exports results
  size(Gx)
#+end_src

#+RESULTS:
: size(Gx)
: State-space model with 3 outputs, 3 inputs, and 6 states.

The diagonal and off-diagonal elements of $G_x$ are shown in Figure [[fig:gravimeter_jacobian_plant]].

#+begin_src matlab :exports none
  figure;

  % Magnitude
  hold on;
  for i_in = 1:3
      for i_out = [1:i_in-1, i_in+1:3]
          plot(freqs, abs(squeeze(freqresp(Gx(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, abs(squeeze(freqresp(Gx(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
       'DisplayName', '$G_x(i,j)\ i \neq j$');
  set(gca,'ColorOrderIndex',1)
  for i_in_out = 1:3
    plot(freqs, abs(squeeze(freqresp(Gx(i_in_out, i_in_out), freqs, 'Hz'))), 'DisplayName', sprintf('$G_x(%d,%d)$', i_in_out, i_in_out));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  xlabel('Frequency [Hz]'); ylabel('Magnitude');
  legend('location', 'southeast');
  ylim([1e-8, 1e0]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_jacobian_plant.pdf', 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:gravimeter_jacobian_plant
#+caption: Diagonal and off-diagonal elements of $G_x$
#+RESULTS:
[[file:figs/gravimeter_jacobian_plant.png]]

** Decoupling using the SVD
<<sec:gravimeter_svd_decoupling>>

In order to decouple the plant using the SVD, first a real approximation of the plant transfer function matrix as the crossover frequency is required.

Let's compute a real approximation of the complex matrix $H_1$ which corresponds to the the transfer function $G(j\omega_c)$ from forces applied by the actuators to the measured acceleration of the top platform evaluated at the frequency $\omega_c$.
#+begin_src matlab
  wc = 2*pi*10; % Decoupling frequency [rad/s]

  H1 = evalfr(G, j*wc);
#+end_src

The real approximation is computed as follows:
#+begin_src matlab
  D = pinv(real(H1'*H1));
  H1 = pinv(D*real(H1'*diag(exp(j*angle(diag(H1*D*H1.'))/2))));
#+end_src

#+begin_src matlab :exports results :results value table replace :tangle no
  data2orgtable(H1, {}, {}, ' %.2g ');
#+end_src

#+caption: Real approximate of $G$ at the decoupling frequency $\omega_c$
#+RESULTS:
|  0.0092 | -0.0039 |  0.0039 |
| -0.0039 |  0.0048 | 0.00028 |
|  -0.004 |  0.0038 | -0.0038 |
| 8.4e-09 |  0.0025 |  0.0025 |


Now, the Singular Value Decomposition of $H_1$ is performed:
\[ H_1 = U \Sigma V^H \]

#+begin_src matlab
  [U,S,V] = svd(H1);
#+end_src

#+begin_src matlab :exports results :results value table replace :tangle no
  data2orgtable(U, {}, {}, ' %.2f ');
#+end_src

#+caption: $U$ matrix
#+RESULTS:
| -0.78 |  0.26 | -0.53 |  -0.2 |
|   0.4 |  0.61 | -0.04 | -0.68 |
|  0.48 | -0.14 | -0.85 |   0.2 |
|  0.03 |  0.73 |  0.06 |  0.68 |

#+begin_src matlab :exports results :results value table replace :tangle no
  data2orgtable(V, {}, {}, ' %.2f ');
#+end_src

#+caption: $V$ matrix
#+RESULTS:
| -0.79 | 0.11 |  -0.6 |
|  0.51 | 0.67 | -0.54 |
| -0.35 | 0.73 |  0.59 |

The obtained matrices $U$ and $V$ are used to decouple the system as shown in Figure [[fig:gravimeter_decouple_svd]].

#+begin_src latex :file gravimeter_decouple_svd.pdf :tangle no :exports results
  \begin{tikzpicture}
    \node[block] (G) {$\bm{G}$};

    \node[block, left=0.6 of G.west] (V) {$V^{-T}$};
    \node[block, right=0.6 of G.east] (U) {$U^{-1}$};

    % Connections and labels
    \draw[<-] (V.west) -- ++(-1.0, 0) node[above right]{$u$};
    \draw[->] (V.east) -- (G.west) node[above left]{$\tau$};
    \draw[->] (G.east) -- (U.west) node[above left]{$a$};
    \draw[->] (U.east) -- ++( 1.0, 0) node[above left]{$y$};

    \begin{scope}[on background layer]
      \node[fit={(V.south west) (G.north-|U.east)}, fill=black!10!white, draw, dashed, inner sep=14pt] (Gsvd) {};
      \node[below right] at (Gsvd.north west) {$\bm{G}_{SVD}$};
    \end{scope}
  \end{tikzpicture}
#+end_src

#+name: fig:gravimeter_decouple_svd
#+caption: Decoupled plant $\bm{G}_{SVD}$ using the Singular Value Decomposition
#+RESULTS:
[[file:figs/gravimeter_decouple_svd.png]]

The decoupled plant is then:
\[ \bm{G}_{SVD}(s) = U^{-1} \bm{G}(s) V^{-H} \]

#+begin_src matlab
  Gsvd = inv(U)*G*inv(V');
#+end_src

#+begin_src matlab :results output replace :exports results
  size(Gsvd)
#+end_src

#+RESULTS:
: size(Gsvd)
: State-space model with 4 outputs, 3 inputs, and 6 states.

The 4th output (corresponding to the null singular value) is discarded, and we only keep the $3 \times 3$ plant:
#+begin_src matlab
  Gsvd = Gsvd(1:3, 1:3);
#+end_src

The diagonal and off-diagonal elements of the "SVD" plant are shown in Figure [[fig:gravimeter_svd_plant]].
#+begin_src matlab :exports none
  figure;

  % Magnitude
  hold on;
  for i_in = 1:3
      for i_out = [1:i_in-1, i_in+1:3]
          plot(freqs, abs(squeeze(freqresp(Gsvd(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, abs(squeeze(freqresp(Gsvd(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
       'DisplayName', '$G_x(i,j)\ i \neq j$');
  set(gca,'ColorOrderIndex',1)
  for i_in_out = 1:3
    plot(freqs, abs(squeeze(freqresp(Gsvd(i_in_out, i_in_out), freqs, 'Hz'))), 'DisplayName', sprintf('$G_x(%d,%d)$', i_in_out, i_in_out));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  xlabel('Frequency [Hz]'); ylabel('Magnitude');
  legend('location', 'southwest', 'FontSize', 8);
  ylim([1e-8, 1e0]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_svd_plant.pdf', 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:gravimeter_svd_plant
#+caption: Diagonal and off-diagonal elements of $G_{svd}$
#+RESULTS:
[[file:figs/gravimeter_svd_plant.png]]

** Verification of the decoupling using the "Gershgorin Radii"
<<sec:gravimeter_gershgorin_radii>>

The "Gershgorin Radii" is computed for the coupled plant $G(s)$, for the "Jacobian plant" $G_x(s)$ and the "SVD Decoupled Plant" $G_{SVD}(s)$:

The "Gershgorin Radii" of a matrix $S$ is defined by:
\[ \zeta_i(j\omega) = \frac{\sum\limits_{j\neq i}|S_{ij}(j\omega)|}{|S_{ii}(j\omega)|} \]

#+begin_src matlab :exports none
  % Gershgorin Radii for the coupled plant:
  Gr_coupled = zeros(length(freqs), size(G,2));
  H = abs(squeeze(freqresp(G, freqs, 'Hz')));
  for out_i = 1:size(G,2)
      Gr_coupled(:, out_i) = squeeze((sum(H(out_i,:,:)) - H(out_i,out_i,:))./H(out_i, out_i, :));
  end

  % Gershgorin Radii for the decoupled plant using SVD:
  Gr_decoupled = zeros(length(freqs), size(Gsvd,2));
  H = abs(squeeze(freqresp(Gsvd, freqs, 'Hz')));
  for out_i = 1:size(Gsvd,2)
      Gr_decoupled(:, out_i) = squeeze((sum(H(out_i,:,:)) - H(out_i,out_i,:))./H(out_i, out_i, :));
  end

  % Gershgorin Radii for the decoupled plant using the Jacobian:
  Gr_jacobian = zeros(length(freqs), size(Gx,2));
  H = abs(squeeze(freqresp(Gx, freqs, 'Hz')));
  for out_i = 1:size(Gx,2)
      Gr_jacobian(:, out_i) = squeeze((sum(H(out_i,:,:)) - H(out_i,out_i,:))./H(out_i, out_i, :));
  end
#+end_src

#+begin_src matlab :exports results
  figure;
  hold on;
  plot(freqs, Gr_coupled(:,1), 'DisplayName', 'Coupled');
  plot(freqs, Gr_decoupled(:,1), 'DisplayName', 'SVD');
  plot(freqs, Gr_jacobian(:,1), 'DisplayName', 'Jacobian');
  for in_i = 2:3
      set(gca,'ColorOrderIndex',1)
      plot(freqs, Gr_coupled(:,in_i), 'HandleVisibility', 'off');
      set(gca,'ColorOrderIndex',2)
      plot(freqs, Gr_decoupled(:,in_i), 'HandleVisibility', 'off');
      set(gca,'ColorOrderIndex',3)
      plot(freqs, Gr_jacobian(:,in_i), 'HandleVisibility', 'off');
  end
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  hold off;
  xlabel('Frequency (Hz)'); ylabel('Gershgorin Radii')
  legend('location', 'southwest');
  ylim([1e-4, 1e2]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_gershgorin_radii.pdf', 'eps', true, 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:gravimeter_gershgorin_radii
#+caption: Gershgorin Radii of the Coupled and Decoupled plants
#+RESULTS:
[[file:figs/gravimeter_gershgorin_radii.png]]

** Verification of the decoupling using the "Relative Gain Array"
<<sec:gravimeter_rga>>

The relative gain array (RGA) is defined as:
\begin{equation}
  \Lambda\big(G(s)\big) = G(s) \times \big( G(s)^{-1} \big)^T
\end{equation}
where $\times$ denotes an element by element multiplication and $G(s)$ is an $n \times n$ square transfer matrix.

The obtained RGA elements are shown in Figure [[fig:gravimeter_rga]].

#+begin_src matlab :exports none
  % Relative Gain Array for the decoupled plant using SVD:
  RGA_svd = zeros(length(freqs), size(Gsvd,1), size(Gsvd,2));
  Gsvd_inv = inv(Gsvd);
  for f_i = 1:length(freqs)
    RGA_svd(f_i, :, :) = abs(evalfr(Gsvd, j*2*pi*freqs(f_i)).*evalfr(Gsvd_inv, j*2*pi*freqs(f_i))');
  end

  % Relative Gain Array for the decoupled plant using the Jacobian:
  RGA_x = zeros(length(freqs), size(Gx,1), size(Gx,2));
  Gx_inv = inv(Gx);
  for f_i = 1:length(freqs)
    RGA_x(f_i, :, :) = abs(evalfr(Gx, j*2*pi*freqs(f_i)).*evalfr(Gx_inv, j*2*pi*freqs(f_i))');
  end
#+end_src

#+begin_src matlab :exports none
  figure;
  tiledlayout(1, 2, 'TileSpacing', 'None', 'Padding', 'None');

  ax1 = nexttile;
  hold on;
  for i_in = 1:3
      for i_out = [1:i_in-1, i_in+1:3]
          plot(freqs, RGA_svd(:, i_out, i_in), '--', 'color', [0 0 0 0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, RGA_svd(:, 1, 2), '--', 'color', [0 0 0 0.2], ...
       'DisplayName', '$RGA_{SVD}(i,j),\ i \neq j$');

  plot(freqs, RGA_svd(:, 1, 1), 'k-', ...
       'DisplayName', '$RGA_{SVD}(i,i)$');
  for ch_i = 1:3
    plot(freqs, RGA_svd(:, ch_i, ch_i), 'k-', ...
         'HandleVisibility', 'off');
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('Magnitude'); xlabel('Frequency [Hz]');
  legend('location', 'southwest');

  ax2 = nexttile;
  hold on;
  for i_in = 1:3
      for i_out = [1:i_in-1, i_in+1:3]
          plot(freqs, RGA_x(:, i_out, i_in), '--', 'color', [0 0 0 0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, RGA_x(:, 1, 2), '--', 'color', [0 0 0 0.2], ...
       'DisplayName', '$RGA_{X}(i,j),\ i \neq j$');

  plot(freqs, RGA_x(:, 1, 1), 'k-', ...
       'DisplayName', '$RGA_{X}(i,i)$');
  for ch_i = 1:3
    plot(freqs, RGA_x(:, ch_i, ch_i), 'k-', ...
         'HandleVisibility', 'off');
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  xlabel('Frequency [Hz]'); set(gca, 'YTickLabel',[]);
  legend('location', 'southwest');

  linkaxes([ax1,ax2],'y');
  ylim([1e-5, 1e1]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_rga.pdf', 'width', 'wide', 'height', 'tall');
#+end_src

#+name: fig:gravimeter_rga
#+caption: Obtained norm of RGA elements for the SVD decoupled plant and the Jacobian decoupled plant
#+RESULTS:
[[file:figs/gravimeter_rga.png]]

The RGA-number is also a measure of diagonal dominance:
\begin{equation}
  \text{RGA-number} = \| \Lambda(G) - I \|_\text{sum}
\end{equation}

#+begin_src matlab :exports none
  % Relative Gain Array for the decoupled plant using SVD:
  RGA_svd = zeros(size(Gsvd,1), size(Gsvd,2), length(freqs));
  Gsvd_inv = inv(Gsvd);
  for f_i = 1:length(freqs)
    RGA_svd(:, :, f_i) = abs(evalfr(Gsvd, j*2*pi*freqs(f_i)).*evalfr(Gsvd_inv, j*2*pi*freqs(f_i))');
  end

  % Relative Gain Array for the decoupled plant using the Jacobian:
  RGA_x = zeros(size(Gx,1), size(Gx,2), length(freqs));
  Gx_inv = inv(Gx);
  for f_i = 1:length(freqs)
    RGA_x(:, :, f_i) = abs(evalfr(Gx, j*2*pi*freqs(f_i)).*evalfr(Gx_inv, j*2*pi*freqs(f_i))');
  end
#+end_src

#+begin_src matlab :exports none
  RGA_num_svd = squeeze(sum(sum(RGA_svd - eye(3))));
  RGA_num_x = squeeze(sum(sum(RGA_x - eye(3))));

  figure;
  hold on;
  plot(freqs, RGA_num_svd)
  plot(freqs, RGA_num_x)
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  xlabel('Frequency [Hz]'); ylabel('RGA-Number');
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_rga_num.pdf', 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:gravimeter_rga_num
#+caption: RGA-Number for the Gravimeter
#+RESULTS:
[[file:figs/gravimeter_rga_num.png]]

** Obtained Decoupled Plants
<<sec:gravimeter_decoupled_plant>>

The bode plot of the diagonal and off-diagonal elements of $G_{SVD}$ are shown in Figure [[fig:gravimeter_decoupled_plant_svd]].

#+begin_src matlab :exports none
  figure;
  tiledlayout(3, 1, 'TileSpacing', 'None', 'Padding', 'None');

  % Magnitude
  ax1 = nexttile([2, 1]);
  hold on;
  for i_in = 1:3
      for i_out = [1:i_in-1, i_in+1:3]
          plot(freqs, abs(squeeze(freqresp(Gsvd(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, abs(squeeze(freqresp(Gsvd(1, 2), freqs, 'Hz'))), 'color', [0,0,0,0.5], ...
       'DisplayName', '$G_{SVD}(i,j),\ i \neq j$');
  set(gca,'ColorOrderIndex',1)
  for ch_i = 1:3
    plot(freqs, abs(squeeze(freqresp(Gsvd(ch_i, ch_i), freqs, 'Hz'))), ...
         'DisplayName', sprintf('$G_{SVD}(%i,%i)$', ch_i, ch_i));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('Magnitude'); set(gca, 'XTickLabel',[]);
  legend('location', 'southwest');
  ylim([1e-8, 1e0])

  % Phase
  ax2 = nexttile;
  hold on;
  for ch_i = 1:3
    plot(freqs, 180/pi*angle(squeeze(freqresp(Gsvd(ch_i, ch_i), freqs, 'Hz'))));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'lin');
  ylabel('Phase [deg]'); xlabel('Frequency [Hz]');
  ylim([-180, 180]);
  yticks([-180:90:360]);

  linkaxes([ax1,ax2],'x');
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_decoupled_plant_svd.pdf', 'eps', true, 'width', 'wide', 'height', 'tall');
#+end_src

#+name: fig:gravimeter_decoupled_plant_svd
#+caption: Decoupled Plant using SVD
#+RESULTS:
[[file:figs/gravimeter_decoupled_plant_svd.png]]

Similarly, the bode plots of the diagonal elements and off-diagonal elements of the decoupled plant $G_x(s)$ using the Jacobian are shown in Figure [[fig:gravimeter_decoupled_plant_jacobian]].

#+begin_src matlab :exports none
  figure;
  tiledlayout(3, 1, 'TileSpacing', 'None', 'Padding', 'None');

  % Magnitude
  ax1 = nexttile([2, 1]);
  hold on;
  for i_in = 1:3
      for i_out = [1:i_in-1, i_in+1:3]
          plot(freqs, abs(squeeze(freqresp(Gx(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, abs(squeeze(freqresp(Gx(1, 2), freqs, 'Hz'))), 'color', [0,0,0,0.5], ...
       'DisplayName', '$G_x(i,j),\ i \neq j$');
  set(gca,'ColorOrderIndex',1)
  plot(freqs, abs(squeeze(freqresp(Gx(1, 1), freqs, 'Hz'))), 'DisplayName', '$G_x(1,1) = A_x/F_x$');
  plot(freqs, abs(squeeze(freqresp(Gx(2, 2), freqs, 'Hz'))), 'DisplayName', '$G_x(2,2) = A_y/F_y$');
  plot(freqs, abs(squeeze(freqresp(Gx(3, 3), freqs, 'Hz'))), 'DisplayName', '$G_x(3,3) = R_z/M_z$');
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('Magnitude'); set(gca, 'XTickLabel',[]);
  legend('location', 'southwest');
  ylim([1e-8, 1e0])

  % Phase
  ax2 = nexttile;
  hold on;
  plot(freqs, 180/pi*angle(squeeze(freqresp(Gx(1, 1), freqs, 'Hz'))));
  plot(freqs, 180/pi*angle(squeeze(freqresp(Gx(2, 2), freqs, 'Hz'))));
  plot(freqs, 180/pi*angle(squeeze(freqresp(Gx(3, 3), freqs, 'Hz'))));
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'lin');
  ylabel('Phase [deg]'); xlabel('Frequency [Hz]');
  ylim([-180, 180]);
  yticks([0:45:360]);

  linkaxes([ax1,ax2],'x');
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_decoupled_plant_jacobian.pdf', 'eps', true, 'width', 'wide', 'height', 'tall');
#+end_src

#+name: fig:gravimeter_decoupled_plant_jacobian
#+caption: Gravimeter Platform Plant from forces (resp. torques) applied by the legs to the acceleration (resp. angular acceleration) of the platform as well as all the coupling terms between the two (non-diagonal terms of the transfer function matrix)
#+RESULTS:
[[file:figs/gravimeter_decoupled_plant_jacobian.png]]

** Diagonal Controller
<<sec:gravimeter_diagonal_control>>
The control diagram for the centralized control is shown in Figure [[fig:centralized_control_gravimeter]].

The controller $K_c$ is "working" in an cartesian frame.
The Jacobian is used to convert forces in the cartesian frame to forces applied by the actuators.

#+begin_src latex :file centralized_control_gravimeter.pdf :tangle no :exports results
  \begin{tikzpicture}
    \node[block] (G) {$\bm{G}$};
    \node[block, left=0.6 of G] (Jt) {$J_{\tau}^{-T}$};
    \node[block, right=0.6 of G] (Ja) {$J_{a}^{-1}$};
    \node[block, left=1.2 of Jt] (K) {$K_c$};

    % Connections and labels
    \draw[->] (Jt.east) -- (G.west)  node[above left]{$\bm{\tau}$};
    \draw[->] (G.east) -- (Ja.west)  node[above left]{$\bm{a}$};
    \draw[->] (Ja.east) -- ++(1.4, 0);
    \draw[->] ($(Ja.east) + (0.8, 0)$) node[branch]{} node[above]{$\bm{\mathcal{A}}$} -- ++(0, -1.2) -| ($(K.west) + (-0.6, 0)$) -- (K.west);
    \draw[->] (K.east) -- (Jt.west) node[above left]{$\bm{\mathcal{F}}$};

    \begin{scope}[on background layer]
      \node[fit={(Jt.south west) (Ja.north east)}, fill=black!10!white, draw, dashed, inner sep=14pt] (Gx) {};
      \node[below right] at (Gx.north west) {$\bm{G}_x$};
    \end{scope}
  \end{tikzpicture}
#+end_src

#+name: fig:centralized_control_gravimeter
#+caption: Control Diagram for the Centralized control
#+RESULTS:
[[file:figs/centralized_control_gravimeter.png]]

The SVD control architecture is shown in Figure [[fig:svd_control_gravimeter]].
The matrices $U$ and $V$ are used to decoupled the plant $G$.

#+begin_src latex :file svd_control_gravimeter.pdf :tangle no :exports results
  \begin{tikzpicture}
    \node[block] (G) {$\bm{G}$};

    \node[block, left=0.6 of G.west] (V) {$V^{-T}$};
    \node[block, right=0.6 of G.east] (U) {$U^{-1}$};
    \node[block, left=1.2 of V] (K) {$K_c$};

    % Connections and labels
    \draw[->] (V.east) -- (G.west) node[above left]{$\tau$};
    \draw[->] (G.east) -- (U.west) node[above left]{$a$};
    \draw[->] (U.east) -- ++( 1.4, 0);
    \draw[->] ($(U.east) + (0.8, 0)$) node[branch]{} node[above]{$y$} -- ++(0, -1.2) -| ($(K.west) + (-0.6, 0)$) -- (K.west);
    \draw[->] (K.east) -- (V.west) node[above left]{$u$};

    \begin{scope}[on background layer]
      \node[fit={(V.south west) (G.north-|U.east)}, fill=black!10!white, draw, dashed, inner sep=14pt] (Gsvd) {};
      \node[below right] at (Gsvd.north west) {$\bm{G}_{SVD}$};
    \end{scope}
  \end{tikzpicture}
#+end_src

#+name: fig:svd_control_gravimeter
#+caption: Control Diagram for the SVD control
#+RESULTS:
[[file:figs/svd_control_gravimeter.png]]


We choose the controller to be a low pass filter:
\[ K_c(s) = \frac{G_0}{1 + \frac{s}{\omega_0}} \]

$G_0$ is tuned such that the crossover frequency corresponding to the diagonal terms of the loop gain is equal to $\omega_c$

#+begin_src matlab
  wc = 2*pi*10;  % Crossover Frequency [rad/s]
  w0 = 2*pi*0.1; % Controller Pole [rad/s]
#+end_src

#+begin_src matlab
  K_cen = diag(1./diag(abs(evalfr(Gx, j*wc))))*(1/abs(evalfr(1/(1 + s/w0), j*wc)))/(1 + s/w0);
  L_cen = K_cen*Gx;
  G_cen = feedback(G, pinv(Jt')*K_cen*pinv(Ja));
#+end_src

#+begin_src matlab
  K_svd = diag(1./diag(abs(evalfr(Gsvd, j*wc))))*(1/abs(evalfr(1/(1 + s/w0), j*wc)))/(1 + s/w0);
  L_svd = K_svd*Gsvd;
  U_inv = inv(U);
  G_svd = feedback(G, inv(V')*K_svd*U_inv(1:3, :));
#+end_src

The obtained diagonal elements of the loop gains are shown in Figure [[fig:gravimeter_comp_loop_gain_diagonal]].

#+begin_src matlab :exports none
  figure;
  tiledlayout(3, 1, 'TileSpacing', 'None', 'Padding', 'None');

  % Magnitude
  ax1 = nexttile([2, 1]);
  hold on;
  plot(freqs, abs(squeeze(freqresp(L_svd(1, 1), freqs, 'Hz'))), 'DisplayName', '$L_{SVD}(i,i)$');
  for i_in_out = 2:3
    set(gca,'ColorOrderIndex',1)
    plot(freqs, abs(squeeze(freqresp(L_svd(i_in_out, i_in_out), freqs, 'Hz'))), 'HandleVisibility', 'off');
  end

  set(gca,'ColorOrderIndex',2)
  plot(freqs, abs(squeeze(freqresp(L_cen(1, 1), freqs, 'Hz'))), ...
       'DisplayName', '$L_{J}(i,i)$');
  for i_in_out = 2:3
    set(gca,'ColorOrderIndex',2)
    plot(freqs, abs(squeeze(freqresp(L_cen(i_in_out, i_in_out), freqs, 'Hz'))), 'HandleVisibility', 'off');
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('Magnitude'); set(gca, 'XTickLabel',[]);
  legend('location', 'northwest');
  ylim([5e-2, 2e3])

  % Phase
  ax2 = nexttile;
  hold on;
  for i_in_out = 1:3
    set(gca,'ColorOrderIndex',1)
    plot(freqs, 180/pi*angle(squeeze(freqresp(L_svd(i_in_out, i_in_out), freqs, 'Hz'))));
  end
  set(gca,'ColorOrderIndex',2)
  for i_in_out = 1:3
    set(gca,'ColorOrderIndex',2)
    plot(freqs, 180/pi*angle(squeeze(freqresp(L_cen(i_in_out, i_in_out), freqs, 'Hz'))));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'lin');
  ylabel('Phase [deg]'); xlabel('Frequency [Hz]');
  ylim([-180, 180]);
  yticks([-180:90:360]);

  linkaxes([ax1,ax2],'x');
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_comp_loop_gain_diagonal.pdf', 'width', 'wide', 'height', 'tall');
#+end_src

#+name: fig:gravimeter_comp_loop_gain_diagonal
#+caption: Comparison of the diagonal elements of the loop gains for the SVD control architecture and the Jacobian one
#+RESULTS:
[[file:figs/gravimeter_comp_loop_gain_diagonal.png]]

** Closed-Loop system Performances
<<sec:gravimeter_closed_loop_results>>

Let's first verify the stability of the closed-loop systems:
#+begin_src matlab :results output replace text
  isstable(G_cen)
#+end_src

#+RESULTS:
: ans =
:   logical
:    1

#+begin_src matlab :results output replace text
  isstable(G_svd)
#+end_src

#+RESULTS:
: ans =
:   logical
:    1

The obtained transmissibility in Open-loop, for the centralized control as well as for the SVD control are shown in Figure [[fig:gravimeter_platform_simscape_cl_transmissibility]].

#+begin_src matlab :exports results
  freqs = logspace(-2, 2, 1000);

  figure;
  tiledlayout(1, 3, 'TileSpacing', 'None', 'Padding', 'None');

  ax1 = nexttile;
  hold on;
  plot(freqs, abs(squeeze(freqresp(G(    1,1)/s^2, freqs, 'Hz'))), 'DisplayName', 'Open-Loop');
  plot(freqs, abs(squeeze(freqresp(G_cen(1,1)/s^2, freqs, 'Hz'))), 'DisplayName', 'Centralized');
  plot(freqs, abs(squeeze(freqresp(G_svd(1,1)/s^2, freqs, 'Hz'))), '--', 'DisplayName', 'SVD');
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('Transmissibility'); xlabel('Frequency [Hz]');
  title('$D_x/D_{w,x}$');
  legend('location', 'southwest');

  ax2 = nexttile;
  hold on;
  plot(freqs, abs(squeeze(freqresp(G(    2,2)/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_cen(2,2)/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_svd(2,2)/s^2, freqs, 'Hz'))), '--');
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  set(gca, 'YTickLabel',[]); xlabel('Frequency [Hz]');
  title('$D_y/D_{w,y}$');

  ax3 = nexttile;
  hold on;
  plot(freqs, abs(squeeze(freqresp(G(    3,3)/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_cen(3,3)/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_svd(3,3)/s^2, freqs, 'Hz'))), '--');
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  set(gca, 'YTickLabel',[]); xlabel('Frequency [Hz]');
  title('$R_z/R_{w,z}$');

  linkaxes([ax1,ax2,ax3],'xy');
  xlim([freqs(1), freqs(end)]);
  xlim([1e-2, 5e1]); ylim([1e-7, 1e-2]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_platform_simscape_cl_transmissibility.pdf', 'eps', true, 'width', 'wide', 'height', 'tall');
#+end_src

#+name: fig:gravimeter_platform_simscape_cl_transmissibility
#+caption: Obtained Transmissibility
#+RESULTS:
[[file:figs/gravimeter_platform_simscape_cl_transmissibility.png]]

#+begin_src matlab :exports results
  freqs = logspace(-2, 2, 1000);

  figure;
  hold on;
  for out_i = 1:3
      for in_i = out_i+1:3
          set(gca,'ColorOrderIndex',1)
          plot(freqs, abs(squeeze(freqresp(G(    out_i,in_i), freqs, 'Hz'))));
          set(gca,'ColorOrderIndex',2)
          plot(freqs, abs(squeeze(freqresp(G_cen(out_i,in_i), freqs, 'Hz'))));
          set(gca,'ColorOrderIndex',3)
          plot(freqs, abs(squeeze(freqresp(G_svd(out_i,in_i), freqs, 'Hz'))), '--');
      end
  end
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('Transmissibility'); xlabel('Frequency [Hz]');
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_cl_transmissibility_coupling.pdf', 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:gravimeter_cl_transmissibility_coupling
#+caption: Obtain coupling terms of the transmissibility matrix
#+RESULTS:
[[file:figs/gravimeter_cl_transmissibility_coupling.png]]


** Robustness to a change of actuator position

Let say we change the position of the actuators:
#+begin_src matlab
  la = l/2*0.7; % Position of Act. [m]
  ha = h/2*0.7; % Position of Act. [m]
#+end_src

#+begin_src matlab :exports none
  %% Name of the Simulink File
  mdl = 'gravimeter';

  %% Input/Output definition
  clear io; io_i = 1;
  io(io_i) = linio([mdl, '/F1'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/F2'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/F3'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_side'], 1, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_side'], 2, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_top'], 1, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_top'], 2, 'openoutput'); io_i = io_i + 1;

  G = linearize(mdl, io);
  G.InputName  = {'F1', 'F2', 'F3'};
  G.OutputName = {'Ax1', 'Ay1', 'Ax2', 'Ay2'};
#+end_src

#+begin_src matlab :exports none
  G_cen_b = feedback(G, pinv(Jt')*K_cen*pinv(Ja));
  G_svd_b = feedback(G, inv(V')*K_svd*U_inv(1:3, :));
#+end_src

The new plant is computed, and the centralized and SVD control architectures are applied using the previsouly computed Jacobian matrices and $U$ and $V$ matrices.

The closed-loop system are still stable, and their

#+begin_src matlab :exports results
  freqs = logspace(-2, 2, 1000);

  figure;
  tiledlayout(1, 3, 'TileSpacing', 'None', 'Padding', 'None');

  ax1 = nexttile;
  hold on;
  plot(freqs, abs(squeeze(freqresp(G_cen(1,1)/s^2, freqs, 'Hz'))), 'DisplayName', 'Initial');
  plot(freqs, abs(squeeze(freqresp(G_cen_b(1,1)/s^2, freqs, 'Hz'))), 'DisplayName', 'Jacobian');
  plot(freqs, abs(squeeze(freqresp(G_svd_b(1,1)/s^2, freqs, 'Hz'))), '--', 'DisplayName', 'SVD');
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('Transmissibility'); xlabel('Frequency [Hz]');
  title('$D_x/D_{w,x}$');
  legend('location', 'southwest');

  ax2 = nexttile;
  hold on;
  plot(freqs, abs(squeeze(freqresp(G_cen(2,2)/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_cen_b(2,2)/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_svd_b(2,2)/s^2, freqs, 'Hz'))), '--');
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  set(gca, 'YTickLabel',[]); xlabel('Frequency [Hz]');
  title('$D_y/D_{w,y}$');

  ax3 = nexttile;
  hold on;
  plot(freqs, abs(squeeze(freqresp(G_cen(3,3)/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_cen_b(3,3)/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_svd_b(3,3)/s^2, freqs, 'Hz'))), '--');
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  set(gca, 'YTickLabel',[]); xlabel('Frequency [Hz]');
  title('$R_z/R_{w,z}$');

  linkaxes([ax1,ax2,ax3],'xy');
  xlim([freqs(1), freqs(end)]);
  xlim([1e-2, 5e1]); ylim([1e-7, 3e-4]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_transmissibility_offset_act.pdf', 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:gravimeter_transmissibility_offset_act
#+caption: Transmissibility for the initial CL system and when the position of  actuators are changed
#+RESULTS:
[[file:figs/gravimeter_transmissibility_offset_act.png]]

** Combined / comparison of K and M decoupling
*** Introduction                                                    :ignore:

If we want to decouple the system at low frequency (determined by the stiffness matrix), we have to compute the Jacobians at a point where the stiffness matrix is diagonal.
A displacement (resp. rotation) of the mass at this particular point should induce a *pure* force (resp. torque) on the same point due to stiffnesses in the system.
This can be verified by geometrical computations.


If we want to decouple the system at high frequency (determined by the mass matrix), we have tot compute the Jacobians at the Center of Mass of the suspended solid.
Similarly to the stiffness analysis, when considering only the inertia effects (neglecting the stiffnesses), a force (resp. torque) applied at this point (the center of mass) should induce a *pure* acceleration (resp. angular acceleration).


Ideally, we would like to have a decoupled mass matrix and stiffness matrix at the same time.
To do so, the actuators (springs) should be positioned such that the stiffness matrix is diagonal when evaluated at the CoM of the solid.

*** Decoupling of the mass matrix

#+name: fig:gravimeter_model_M
#+caption: Choice of {O} such that the Mass Matrix is Diagonal
[[file:figs/gravimeter_model_M.png]]

#+begin_src matlab
  la = l/2; % Position of Act. [m]
  ha = h/2; % Position of Act. [m]
#+end_src

#+begin_src matlab
  %% Name of the Simulink File
  mdl = 'gravimeter';

  %% Input/Output definition
  clear io; io_i = 1;
  io(io_i) = linio([mdl, '/F1'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/F2'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/F3'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_side'], 1, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_side'], 2, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_top'], 1, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_top'], 2, 'openoutput'); io_i = io_i + 1;

  G = linearize(mdl, io);
  G.InputName  = {'F1', 'F2', 'F3'};
  G.OutputName = {'Ax1', 'Ay1', 'Ax2', 'Ay2'};
#+end_src

Decoupling at the CoM (Mass decoupled)
#+begin_src matlab
  JMa = [1 0 -h/2
         0 1  l/2
         1 0  h/2
         0 1  0];

  JMt = [1 0 -ha
         0 1  la
         0 1 -la];
#+end_src

#+begin_src matlab
  GM = pinv(JMa)*G*pinv(JMt');
  GM.InputName  = {'Fx', 'Fy', 'Mz'};
  GM.OutputName  = {'Dx', 'Dy', 'Rz'};
#+end_src

#+begin_src matlab :exports none
  figure;

  % Magnitude
  hold on;
  for i_in = 1:3
      for i_out = [1:i_in-1, i_in+1:3]
          plot(freqs, abs(squeeze(freqresp(GM(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, abs(squeeze(freqresp(GM(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
       'DisplayName', '$G_x(i,j)\ i \neq j$');
  set(gca,'ColorOrderIndex',1)
  for i_in_out = 1:3
    plot(freqs, abs(squeeze(freqresp(GM(i_in_out, i_in_out), freqs, 'Hz'))), 'DisplayName', sprintf('$G_x(%d,%d)$', i_in_out, i_in_out));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  xlabel('Frequency [Hz]'); ylabel('Magnitude');
  legend('location', 'southeast');
  ylim([1e-8, 1e0]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/jac_decoupling_M.pdf', 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:jac_decoupling_M
#+caption: Diagonal and off-diagonal elements of the decoupled plant
#+RESULTS:
[[file:figs/jac_decoupling_M.png]]

*** Decoupling of the stiffness matrix

#+name: fig:gravimeter_model_K
#+caption: Choice of {O} such that the Stiffness Matrix is Diagonal
[[file:figs/gravimeter_model_K.png]]

Decoupling at the point where K is diagonal (x = 0, y = -h/2 from the schematic {O} frame):
#+begin_src matlab
  JKa = [1 0  0
         0 1 -l/2
         1 0 -h
         0 1  0];

  JKt = [1 0  0
         0 1 -la
         0 1  la];
#+end_src

And the plant $\bm{G}_x$ is computed:
#+begin_src matlab
  GK = pinv(JKa)*G*pinv(JKt');
  GK.InputName  = {'Fx', 'Fy', 'Mz'};
  GK.OutputName  = {'Dx', 'Dy', 'Rz'};
#+end_src

#+begin_src matlab :exports none
  figure;

  % Magnitude
  hold on;
  for i_in = 1:3
      for i_out = [1:i_in-1, i_in+1:3]
          plot(freqs, abs(squeeze(freqresp(GK(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, abs(squeeze(freqresp(GK(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
       'DisplayName', '$G_x(i,j)\ i \neq j$');
  set(gca,'ColorOrderIndex',1)
  for i_in_out = 1:3
    plot(freqs, abs(squeeze(freqresp(GK(i_in_out, i_in_out), freqs, 'Hz'))), 'DisplayName', sprintf('$G_x(%d,%d)$', i_in_out, i_in_out));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  xlabel('Frequency [Hz]'); ylabel('Magnitude');
  legend('location', 'southeast');
  ylim([1e-8, 1e0]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/jac_decoupling_K.pdf', 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:jac_decoupling_K
#+caption: Diagonal and off-diagonal elements of the decoupled plant
#+RESULTS:
[[file:figs/jac_decoupling_K.png]]

*** Combined decoupling of the mass and stiffness matrices

#+name: fig:gravimeter_model_KM
#+caption: Ideal location of the actuators such that both the mass and stiffness matrices are diagonal
[[file:figs/gravimeter_model_KM.png]]

To do so, the actuator position should be modified

#+begin_src matlab
  la = l/2; % Position of Act. [m]
  ha = 0; % Position of Act. [m]
#+end_src

#+begin_src matlab
  %% Name of the Simulink File
  mdl = 'gravimeter';

  %% Input/Output definition
  clear io; io_i = 1;
  io(io_i) = linio([mdl, '/F1'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/F2'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/F3'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_side'], 1, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_side'], 2, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_top'], 1, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_top'], 2, 'openoutput'); io_i = io_i + 1;

  G = linearize(mdl, io);
  G.InputName  = {'F1', 'F2', 'F3'};
  G.OutputName = {'Ax1', 'Ay1', 'Ax2', 'Ay2'};
#+end_src

#+begin_src matlab
  JMa = [1 0 -h/2
         0 1  l/2
         1 0  h/2
         0 1  0];

  JMt = [1 0 -ha
         0 1  la
         0 1 -la];
#+end_src

#+begin_src matlab
  GKM = pinv(JMa)*G*pinv(JMt');
  GKM.InputName  = {'Fx', 'Fy', 'Mz'};
  GKM.OutputName  = {'Dx', 'Dy', 'Rz'};
#+end_src

#+begin_src matlab :exports none
  figure;

  % Magnitude
  hold on;
  for i_in = 1:3
      for i_out = [1:i_in-1, i_in+1:3]
          plot(freqs, abs(squeeze(freqresp(GKM(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, abs(squeeze(freqresp(GKM(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
       'DisplayName', '$G_x(i,j)\ i \neq j$');
  set(gca,'ColorOrderIndex',1)
  for i_in_out = 1:3
    plot(freqs, abs(squeeze(freqresp(GKM(i_in_out, i_in_out), freqs, 'Hz'))), 'DisplayName', sprintf('$G_x(%d,%d)$', i_in_out, i_in_out));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  xlabel('Frequency [Hz]'); ylabel('Magnitude');
  legend('location', 'southeast');
  ylim([1e-8, 1e0]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/jac_decoupling_KM.pdf', 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:jac_decoupling_KM
#+caption: Diagonal and off-diagonal elements of the decoupled plant
#+RESULTS:
[[file:figs/jac_decoupling_KM.png]]

*** Conclusion

Ideally, the mechanical system should be designed in order to have a decoupled stiffness matrix at the CoM of the solid.

If not the case, the system can either be decoupled as low frequency if the Jacobian are evaluated at a point where the stiffness matrix is decoupled.
Or it can be decoupled at high frequency if the Jacobians are evaluated at the CoM.

** SVD decoupling performances
As the SVD is applied on a *real approximation* of the plant dynamics at a frequency $\omega_0$, it is foreseen that the effectiveness of the decoupling depends on the validity of the real approximation.

Let's do the SVD decoupling on a plant that is mostly real (low damping) and one with a large imaginary part (larger damping).

Start with small damping, the obtained diagonal and off-diagonal terms are shown in Figure [[fig:gravimeter_svd_low_damping]].
#+begin_src matlab
  c = 2e1; % Actuator Damping [N/(m/s)]
#+end_src

#+begin_src matlab :exports none
  %% Name of the Simulink File
  mdl = 'gravimeter';

  %% Input/Output definition
  clear io; io_i = 1;
  io(io_i) = linio([mdl, '/F1'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/F2'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/F3'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_side'], 1, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_side'], 2, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_top'], 1, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_top'], 2, 'openoutput'); io_i = io_i + 1;

  G = linearize(mdl, io);
  G.InputName  = {'F1', 'F2', 'F3'};
  G.OutputName = {'Ax1', 'Ay1', 'Ax2', 'Ay2'};

  wc = 2*pi*10; % Decoupling frequency [rad/s]
  H1 = evalfr(G, j*wc);
  D = pinv(real(H1'*H1));
  H1 = pinv(D*real(H1'*diag(exp(j*angle(diag(H1*D*H1.'))/2))));
  [U,S,V] = svd(H1);
  Gsvd = inv(U)*G*inv(V');
#+end_src

#+begin_src matlab :exports none
  figure;

  % Magnitude
  hold on;
  for i_in = 1:3
      for i_out = [1:i_in-1, i_in+1:3]
          plot(freqs, abs(squeeze(freqresp(Gsvd(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, abs(squeeze(freqresp(Gsvd(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
       'DisplayName', '$G_{svd}(i,j)\ i \neq j$');
  set(gca,'ColorOrderIndex',1)
  for i_in_out = 1:3
    plot(freqs, abs(squeeze(freqresp(Gsvd(i_in_out, i_in_out), freqs, 'Hz'))), 'DisplayName', sprintf('$G_{svd}(%d,%d)$', i_in_out, i_in_out));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  xlabel('Frequency [Hz]'); ylabel('Magnitude');
  legend('location', 'northwest');
  ylim([1e-8, 1e0]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_svd_low_damping.pdf', 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:gravimeter_svd_low_damping
#+caption: Diagonal and off-diagonal term when decoupling with SVD on the gravimeter with small damping
#+RESULTS:
[[file:figs/gravimeter_svd_low_damping.png]]

Now take a larger damping, the obtained diagonal and off-diagonal terms are shown in Figure [[fig:gravimeter_svd_high_damping]].
#+begin_src matlab
  c = 5e2; % Actuator Damping [N/(m/s)]
#+end_src

#+begin_src matlab :exports none
  %% Name of the Simulink File
  mdl = 'gravimeter';

  %% Input/Output definition
  clear io; io_i = 1;
  io(io_i) = linio([mdl, '/F1'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/F2'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/F3'], 1, 'openinput');  io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_side'], 1, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_side'], 2, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_top'], 1, 'openoutput'); io_i = io_i + 1;
  io(io_i) = linio([mdl, '/Acc_top'], 2, 'openoutput'); io_i = io_i + 1;

  G = linearize(mdl, io);
  G.InputName  = {'F1', 'F2', 'F3'};
  G.OutputName = {'Ax1', 'Ay1', 'Ax2', 'Ay2'};

  wc = 2*pi*10; % Decoupling frequency [rad/s]
  H1 = evalfr(G, j*wc);
  D = pinv(real(H1'*H1));
  H1 = pinv(D*real(H1'*diag(exp(j*angle(diag(H1*D*H1.'))/2))));
  [U,S,V] = svd(H1);
  Gsvdd = inv(U)*G*inv(V');
#+end_src

#+begin_src matlab :exports none
  figure;

  % Magnitude
  hold on;
  for i_in = 1:3
      for i_out = [1:i_in-1, i_in+1:3]
          plot(freqs, abs(squeeze(freqresp(Gsvdd(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, abs(squeeze(freqresp(Gsvdd(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
       'DisplayName', '$G_{svd}(i,j)\ i \neq j$');
  set(gca,'ColorOrderIndex',1)
  for i_in_out = 1:3
    plot(freqs, abs(squeeze(freqresp(Gsvdd(i_in_out, i_in_out), freqs, 'Hz'))), 'DisplayName', sprintf('$G_{svd}(%d,%d)$', i_in_out, i_in_out));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  xlabel('Frequency [Hz]'); ylabel('Magnitude');
  legend('location', 'northwest');
  ylim([1e-8, 1e0]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/gravimeter_svd_high_damping.pdf', 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:gravimeter_svd_high_damping
#+caption: Diagonal and off-diagonal term when decoupling with SVD on the gravimeter with high damping
#+RESULTS:
[[file:figs/gravimeter_svd_high_damping.png]]

* Stewart Platform - Simscape Model
:PROPERTIES:
:header-args:matlab+: :tangle stewart_platform/script.m
:END:
<<sec:stewart_platform>>

** Introduction                                                      :ignore:

In this analysis, we wish to applied SVD control to the Stewart Platform shown in Figure [[fig:SP_assembly]].

Some notes about the system:
- 6 voice coils actuators are used to control the motion of the top platform.
- the motion of the top platform is measured with a 6-axis inertial unit (3 acceleration + 3 angular accelerations)
- the control objective is to isolate the top platform from vibrations coming from the bottom platform

#+name: fig:SP_assembly
#+caption: Stewart Platform CAD View
[[file:figs/SP_assembly.png]]

The analysis of the SVD/Jacobian control applied to the Stewart platform is performed in the following sections:
- Section [[sec:stewart_simscape]]: The parameters of the Simscape model of the Stewart platform are defined
- Section [[sec:stewart_identification]]: The plant is identified from the Simscape model and the system coupling is shown
- Section [[sec:stewart_jacobian_decoupling]]: The plant is first decoupled using the Jacobian
- Section [[sec:stewart_svd_decoupling]]: The decoupling is performed thanks to the SVD. To do so a real approximation of the plant is computed.
- Section [[sec:stewart_gershorin_radii]]: The effectiveness of the decoupling with the Jacobian and SVD are compared using the Gershorin Radii
- Section [[sec:stewart_rga]]:
- Section [[sec:stewart_decoupled_plant]]: The dynamics of the decoupled plants are shown
- Section [[sec:stewart_diagonal_control]]: A diagonal controller is defined to control the decoupled plant
- Section [[sec:stewart_closed_loop_results]]: Finally, the closed loop system properties are studied

** Matlab Init                                              :noexport:ignore:
#+begin_src matlab :tangle no :exports none :results silent :noweb yes :var current_dir=(file-name-directory buffer-file-name)
  <<matlab-dir>>
#+end_src

#+begin_src matlab :exports none :results silent :noweb yes
  <<matlab-init>>
#+end_src

#+begin_src matlab :tangle no
  addpath('stewart_platform');
  addpath('stewart_platform/STEP');
#+end_src

#+begin_src matlab :eval no
  addpath('STEP');
#+end_src

#+begin_src matlab
  freqs = logspace(-1, 2, 1000);
#+end_src

** Jacobian                                                        :noexport:
First, the position of the "joints" (points of force application) are estimated and the Jacobian computed.
#+begin_src matlab :tangle no
  open('drone_platform_jacobian.slx');
#+end_src

#+begin_src matlab :tangle no
  sim('drone_platform_jacobian');
#+end_src

#+begin_src matlab :tangle no
  Aa = [a1.Data(1,:);
        a2.Data(1,:);
        a3.Data(1,:);
        a4.Data(1,:);
        a5.Data(1,:);
        a6.Data(1,:)]';

  Ab = [b1.Data(1,:);
        b2.Data(1,:);
        b3.Data(1,:);
        b4.Data(1,:);
        b5.Data(1,:);
        b6.Data(1,:)]';

  As = (Ab - Aa)./vecnorm(Ab - Aa);

  l = vecnorm(Ab - Aa)';

  J = [As' , cross(Ab, As)'];

  save('stewart_platform/jacobian.mat', 'Aa', 'Ab', 'As', 'l', 'J');
#+end_src

** Simscape Model - Parameters
<<sec:stewart_simscape>>
#+begin_src matlab
  open('drone_platform.slx');
#+end_src

Definition of spring parameters:
#+begin_src matlab
  kx = 0.5*1e3/3; % [N/m]
  ky = 0.5*1e3/3;
  kz = 1e3/3;

  cx = 0.025; % [Nm/rad]
  cy = 0.025;
  cz = 0.025;
#+end_src

We suppose the sensor is perfectly positioned.
#+begin_src matlab
  sens_pos_error = zeros(3,1);
#+end_src

Gravity:
#+begin_src matlab
  g = 0;
#+end_src

We load the Jacobian (previously computed from the geometry):
#+begin_src matlab
  load('jacobian.mat', 'Aa', 'Ab', 'As', 'l', 'J');
#+end_src

We initialize other parameters:
#+begin_src matlab
  U = eye(6);
  V = eye(6);
  Kc = tf(zeros(6));
#+end_src

#+name: fig:stewart_simscape
#+attr_latex: :width \linewidth
#+caption: General view of the Simscape Model
[[file:figs/stewart_simscape.png]]

#+name: fig:stewart_platform_details
#+attr_latex: :width \linewidth
#+caption: Simscape model of the Stewart platform
[[file:figs/stewart_platform_details.png]]

** Identification of the plant
<<sec:stewart_identification>>

The plant shown in Figure [[fig:stewart_platform_plant]] is identified from the Simscape model.

The inputs are:
- $D_w$ translation and rotation of the bottom platform (with respect to the center of mass of the top platform)
- $\tau$ the 6 forces applied by the voice coils

The outputs are the 6 accelerations measured by the inertial unit.

#+begin_src latex :file stewart_platform_plant.pdf :tangle no :exports results
  \begin{tikzpicture}
    \node[block={2cm}{1.5cm}] (G) {$\begin{bmatrix}G_d\\G_u\end{bmatrix}$};
    \node[above] at (G.north) {$\bm{G}$};

    % Inputs of the controllers
    \coordinate[] (inputd) at ($(G.south west)!0.75!(G.north west)$);
    \coordinate[] (inputu) at ($(G.south west)!0.25!(G.north west)$);
    % Connections and labels

    \draw[<-] (inputd) -- ++(-0.8, 0) node[above right]{$D_w$};
    \draw[<-] (inputu) -- ++(-0.8, 0) node[above right]{$\tau$};
    \draw[->] (G.east) -- ++(0.8, 0)  node[above left]{$a$};
  \end{tikzpicture}
#+end_src

#+name: fig:stewart_platform_plant
#+caption: Considered plant $\bm{G} = \begin{bmatrix}G_d\\G_u\end{bmatrix}$. $D_w$ is the translation/rotation of the support, $\tau$ the actuator forces, $a$ the acceleration/angular acceleration of the top platform
#+RESULTS:
[[file:figs/stewart_platform_plant.png]]

#+begin_src matlab
  %% Name of the Simulink File
  mdl = 'drone_platform';

  %% Input/Output definition
  clear io; io_i = 1;
  io(io_i) = linio([mdl, '/Dw'],              1, 'openinput');  io_i = io_i + 1; % Ground Motion
  io(io_i) = linio([mdl, '/V-T'],             1, 'openinput');  io_i = io_i + 1; % Actuator Forces
  io(io_i) = linio([mdl, '/Inertial Sensor'], 1, 'openoutput'); io_i = io_i + 1; % Top platform acceleration

  G = linearize(mdl, io);
  G.InputName  = {'Dwx', 'Dwy', 'Dwz', 'Rwx', 'Rwy', 'Rwz', ...
                  'F1', 'F2', 'F3', 'F4', 'F5', 'F6'};
  G.OutputName = {'Ax', 'Ay', 'Az', 'Arx', 'Ary', 'Arz'};

  % Plant
  Gu = G(:, {'F1', 'F2', 'F3', 'F4', 'F5', 'F6'});
  % Disturbance dynamics
  Gd = G(:, {'Dwx', 'Dwy', 'Dwz', 'Rwx', 'Rwy', 'Rwz'});
#+end_src

There are 24 states (6dof for the bottom platform + 6dof for the top platform).
#+begin_src matlab :results output replace
  size(G)
#+end_src

#+RESULTS:
: State-space model with 6 outputs, 12 inputs, and 24 states.

The elements of the transfer matrix $\bm{G}$ corresponding to the transfer function from actuator forces $\tau$ to the measured acceleration $a$ are shown in Figure [[fig:stewart_platform_coupled_plant]].

One can easily see that the system is strongly coupled.

#+begin_src matlab :exports none
  figure;

  % Magnitude
  hold on;
  for i_in = 1:6
      for i_out = [1:i_in-1, i_in+1:6]
          plot(freqs, abs(squeeze(freqresp(Gu(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, abs(squeeze(freqresp(Gu(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
       'DisplayName', '$G_u(i,j)\ i \neq j$');
  set(gca,'ColorOrderIndex',1)
  for i_in_out = 1:6
    plot(freqs, abs(squeeze(freqresp(Gu(i_in_out, i_in_out), freqs, 'Hz'))), 'DisplayName', sprintf('$G_u(%d,%d)$', i_in_out, i_in_out));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  xlabel('Frequency [Hz]'); ylabel('Magnitude');
  ylim([1e-2, 1e5]);
  legend('location', 'northwest');
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/stewart_platform_coupled_plant.pdf', 'eps', true, 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:stewart_platform_coupled_plant
#+caption: Magnitude of all 36 elements of the transfer function matrix $G_u$
#+RESULTS:
[[file:figs/stewart_platform_coupled_plant.png]]

** Decoupling using the Jacobian
<<sec:stewart_jacobian_decoupling>>
Consider the control architecture shown in Figure [[fig:plant_decouple_jacobian]].
The Jacobian matrix is used to transform forces/torques applied on the top platform to the equivalent forces applied by each actuator.

The Jacobian matrix is computed from the geometry of the platform (position and orientation of the actuators).

#+begin_src matlab :exports results :results value table replace :tangle no
  data2orgtable(J, {}, {}, ' %.3f ');
#+end_src

#+caption: Computed Jacobian Matrix
#+RESULTS:
|  0.811 |    0.0 | 0.584 | -0.018 | -0.008 |  0.025 |
| -0.406 | -0.703 | 0.584 | -0.016 | -0.012 | -0.025 |
| -0.406 |  0.703 | 0.584 |  0.016 | -0.012 |  0.025 |
|  0.811 |    0.0 | 0.584 |  0.018 | -0.008 | -0.025 |
| -0.406 | -0.703 | 0.584 |  0.002 |  0.019 |  0.025 |
| -0.406 |  0.703 | 0.584 | -0.002 |  0.019 | -0.025 |

#+begin_src latex :file plant_decouple_jacobian.pdf :tangle no :exports results
  \begin{tikzpicture}
    \node[block] (G) {$G_u$};
    \node[block, left=0.6 of G] (J) {$J^{-T}$};

    % Connections and labels
    \draw[<-] (J.west) -- ++(-1.0, 0) node[above right]{$\mathcal{F}$};
    \draw[->] (J.east) -- (G.west)  node[above left]{$\tau$};
    \draw[->] (G.east) -- ++( 1.0, 0)  node[above left]{$a$};

    \begin{scope}[on background layer]
      \node[fit={(J.south west) (G.north east)}, fill=black!10!white, draw, dashed, inner sep=14pt] (Gx) {};
      \node[below right] at (Gx.north west) {$\bm{G}_x$};
    \end{scope}
  \end{tikzpicture}
#+end_src

#+name: fig:plant_decouple_jacobian
#+caption: Decoupled plant $\bm{G}_x$ using the Jacobian matrix $J$
#+RESULTS:
[[file:figs/plant_decouple_jacobian.png]]

We define a new plant:
\[ G_x(s) = G(s) J^{-T} \]

$G_x(s)$ correspond to the transfer function from forces and torques applied to the top platform to the absolute acceleration of the top platform.

#+begin_src matlab
  Gx = Gu*inv(J');
  Gx.InputName  = {'Fx', 'Fy', 'Fz', 'Mx', 'My', 'Mz'};
#+end_src

** Decoupling using the SVD
<<sec:stewart_svd_decoupling>>

In order to decouple the plant using the SVD, first a real approximation of the plant transfer function matrix as the crossover frequency is required.

Let's compute a real approximation of the complex matrix $H_1$ which corresponds to the the transfer function $G_u(j\omega_c)$ from forces applied by the actuators to the measured acceleration of the top platform evaluated at the frequency $\omega_c$.
#+begin_src matlab
  wc = 2*pi*30; % Decoupling frequency [rad/s]

  H1 = evalfr(Gu, j*wc);
#+end_src

The real approximation is computed as follows:
#+begin_src matlab
  D = pinv(real(H1'*H1));
  H1 = inv(D*real(H1'*diag(exp(j*angle(diag(H1*D*H1.'))/2))));
#+end_src

#+begin_src matlab :exports results :results value table replace :tangle no
  data2orgtable(H1, {}, {}, ' %.1f ');
#+end_src

#+caption: Real approximate of $G$ at the decoupling frequency $\omega_c$
#+RESULTS:
|    4.4 |   -2.1 |   -2.1 |    4.4 |  -2.4 |   -2.4 |
|   -0.2 |   -3.9 |    3.9 |    0.2 |  -3.8 |    3.8 |
|    3.4 |    3.4 |    3.4 |    3.4 |   3.4 |    3.4 |
| -367.1 | -323.8 |  323.8 |  367.1 |  43.3 |  -43.3 |
| -162.0 | -237.0 | -237.0 | -162.0 | 398.9 |  398.9 |
|  220.6 | -220.6 |  220.6 | -220.6 | 220.6 | -220.6 |


Note that the plant $G_u$ at $\omega_c$ is already an almost real matrix.
This can be seen on the Bode plots where the phase is close to 1.
This can be verified below where only the real value of $G_u(\omega_c)$ is shown

#+begin_src matlab :exports results :results value table replace :tangle no
  data2orgtable(real(evalfr(Gu, j*wc)), {}, {}, ' %.1f ');
#+end_src

#+caption: Real part of $G$ at the decoupling frequency $\omega_c$
#+RESULTS:
|    4.4 |   -2.1 |   -2.1 |    4.4 |  -2.4 |   -2.4 |
|   -0.2 |   -3.9 |    3.9 |    0.2 |  -3.8 |    3.8 |
|    3.4 |    3.4 |    3.4 |    3.4 |   3.4 |    3.4 |
| -367.1 | -323.8 |  323.8 |  367.1 |  43.3 |  -43.3 |
| -162.0 | -237.0 | -237.0 | -162.0 | 398.9 |  398.9 |
|  220.6 | -220.6 |  220.6 | -220.6 | 220.6 | -220.6 |

Now, the Singular Value Decomposition of $H_1$ is performed:
\[ H_1 = U \Sigma V^H \]

#+begin_src matlab
  [U,~,V] = svd(H1);
#+end_src

#+begin_src matlab :exports results :results value table replace :tangle no
  data2orgtable(U, {}, {}, ' %.1g ');
#+end_src

#+caption: Obtained matrix $U$
#+RESULTS:
| -0.005 |  7e-06 |  6e-11 | -3e-06 |     -1 |    0.1 |
| -7e-06 | -0.005 | -9e-09 | -5e-09 |   -0.1 |     -1 |
|  4e-08 | -2e-10 | -6e-11 |     -1 |  3e-06 | -3e-07 |
| -0.002 |     -1 | -5e-06 |  2e-10 | 0.0006 |  0.005 |
|      1 | -0.002 | -1e-08 |  2e-08 | -0.005 | 0.0006 |
| -4e-09 |  5e-06 |     -1 |  6e-11 | -2e-09 | -1e-08 |

#+begin_src matlab :exports results :results value table replace :tangle no
  data2orgtable(V, {}, {}, ' %.1g ');
#+end_src

#+caption: Obtained matrix $V$
#+RESULTS:
| -0.2 |   0.5 | -0.4 | -0.4 |   -0.6 | -0.2 |
| -0.3 |   0.5 |  0.4 | -0.4 |    0.5 |  0.3 |
| -0.3 |  -0.5 | -0.4 | -0.4 |    0.4 | -0.4 |
| -0.2 |  -0.5 |  0.4 | -0.4 |   -0.5 |  0.3 |
|  0.6 | -0.06 | -0.4 | -0.4 |    0.1 |  0.6 |
|  0.6 |  0.06 |  0.4 | -0.4 | -0.006 | -0.6 |

The obtained matrices $U$ and $V$ are used to decouple the system as shown in Figure [[fig:plant_decouple_svd]].

#+begin_src latex :file plant_decouple_svd.pdf :tangle no :exports results
  \begin{tikzpicture}
    \node[block] (G) {$G_u$};

    \node[block, left=0.6 of G.west] (V) {$V^{-T}$};
    \node[block, right=0.6 of G.east] (U) {$U^{-1}$};

    % Connections and labels
    \draw[<-] (V.west) -- ++(-1.0, 0) node[above right]{$u$};
    \draw[->] (V.east) -- (G.west) node[above left]{$\tau$};
    \draw[->] (G.east) -- (U.west) node[above left]{$a$};
    \draw[->] (U.east) -- ++( 1.0, 0) node[above left]{$y$};

    \begin{scope}[on background layer]
      \node[fit={(V.south west) (G.north-|U.east)}, fill=black!10!white, draw, dashed, inner sep=14pt] (Gsvd) {};
      \node[below right] at (Gsvd.north west) {$\bm{G}_{SVD}$};
    \end{scope}
  \end{tikzpicture}
#+end_src

#+name: fig:plant_decouple_svd
#+caption: Decoupled plant $\bm{G}_{SVD}$ using the Singular Value Decomposition
#+RESULTS:
[[file:figs/plant_decouple_svd.png]]

The decoupled plant is then:
\[ G_{SVD}(s) = U^{-1} G_u(s) V^{-H} \]

#+begin_src matlab
  Gsvd = inv(U)*Gu*inv(V');
#+end_src

** Verification of the decoupling using the "Gershgorin Radii"
<<sec:stewart_gershorin_radii>>

The "Gershgorin Radii" is computed for the coupled plant $G(s)$, for the "Jacobian plant" $G_x(s)$ and the "SVD Decoupled Plant" $G_{SVD}(s)$:

The "Gershgorin Radii" of a matrix $S$ is defined by:
\[ \zeta_i(j\omega) = \frac{\sum\limits_{j\neq i}|S_{ij}(j\omega)|}{|S_{ii}(j\omega)|} \]

This is computed over the following frequencies.
#+begin_src matlab :exports none
  % Gershgorin Radii for the coupled plant:
  Gr_coupled = zeros(length(freqs), size(Gu,2));
  H = abs(squeeze(freqresp(Gu, freqs, 'Hz')));
  for out_i = 1:size(Gu,2)
      Gr_coupled(:, out_i) = squeeze((sum(H(out_i,:,:)) - H(out_i,out_i,:))./H(out_i, out_i, :));
  end

  % Gershgorin Radii for the decoupled plant using SVD:
  Gr_decoupled = zeros(length(freqs), size(Gsvd,2));
  H = abs(squeeze(freqresp(Gsvd, freqs, 'Hz')));
  for out_i = 1:size(Gsvd,2)
      Gr_decoupled(:, out_i) = squeeze((sum(H(out_i,:,:)) - H(out_i,out_i,:))./H(out_i, out_i, :));
  end

  % Gershgorin Radii for the decoupled plant using the Jacobian:
  Gr_jacobian = zeros(length(freqs), size(Gx,2));
  H = abs(squeeze(freqresp(Gx, freqs, 'Hz')));
  for out_i = 1:size(Gx,2)
      Gr_jacobian(:, out_i) = squeeze((sum(H(out_i,:,:)) - H(out_i,out_i,:))./H(out_i, out_i, :));
  end
#+end_src

#+begin_src matlab :exports results
  figure;
  hold on;
  plot(freqs, Gr_coupled(:,1), 'DisplayName', 'Coupled');
  plot(freqs, Gr_decoupled(:,1), 'DisplayName', 'SVD');
  plot(freqs, Gr_jacobian(:,1), 'DisplayName', 'Jacobian');
  for in_i = 2:6
      set(gca,'ColorOrderIndex',1)
      plot(freqs, Gr_coupled(:,in_i), 'HandleVisibility', 'off');
      set(gca,'ColorOrderIndex',2)
      plot(freqs, Gr_decoupled(:,in_i), 'HandleVisibility', 'off');
      set(gca,'ColorOrderIndex',3)
      plot(freqs, Gr_jacobian(:,in_i), 'HandleVisibility', 'off');
  end
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  hold off;
  xlabel('Frequency (Hz)'); ylabel('Gershgorin Radii')
  legend('location', 'northwest');
  ylim([1e-3, 1e3]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/simscape_model_gershgorin_radii.pdf', 'eps', true, 'width', 'wide', 'height', 'normal');
#+end_src

#+name: fig:simscape_model_gershgorin_radii
#+caption: Gershgorin Radii of the Coupled and Decoupled plants
#+RESULTS:
[[file:figs/simscape_model_gershgorin_radii.png]]

** Verification of the decoupling using the "Relative Gain Array"
<<sec:stewart_rga>>

The relative gain array (RGA) is defined as:
\begin{equation}
  \Lambda\big(G(s)\big) = G(s) \times \big( G(s)^{-1} \big)^T
\end{equation}
where $\times$ denotes an element by element multiplication and $G(s)$ is an $n \times n$ square transfer matrix.

The obtained RGA elements are shown in Figure [[fig:simscape_model_rga]].

#+begin_src matlab :exports none
  % Relative Gain Array for the coupled plant:
  RGA_coupled = zeros(length(freqs), size(Gu,1), size(Gu,2));
  Gu_inv = inv(Gu);
  for f_i = 1:length(freqs)
    RGA_coupled(f_i, :, :) = abs(evalfr(Gu, j*2*pi*freqs(f_i)).*evalfr(Gu_inv, j*2*pi*freqs(f_i))');
  end

  % Relative Gain Array for the decoupled plant using SVD:
  RGA_svd = zeros(length(freqs), size(Gsvd,1), size(Gsvd,2));
  Gsvd_inv = inv(Gsvd);
  for f_i = 1:length(freqs)
    RGA_svd(f_i, :, :) = abs(evalfr(Gsvd, j*2*pi*freqs(f_i)).*evalfr(Gsvd_inv, j*2*pi*freqs(f_i))');
  end

  % Relative Gain Array for the decoupled plant using the Jacobian:
  RGA_x = zeros(length(freqs), size(Gx,1), size(Gx,2));
  Gx_inv = inv(Gx);
  for f_i = 1:length(freqs)
    RGA_x(f_i, :, :) = abs(evalfr(Gx, j*2*pi*freqs(f_i)).*evalfr(Gx_inv, j*2*pi*freqs(f_i))');
  end
#+end_src

#+begin_src matlab :exports none
  figure;
  tiledlayout(1, 2, 'TileSpacing', 'None', 'Padding', 'None');

  ax1 = nexttile;
  hold on;
  for i_in = 1:6
      for i_out = [1:i_in-1, i_in+1:6]
          plot(freqs, RGA_svd(:, i_out, i_in), '--', 'color', [0 0 0 0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, RGA_svd(:, 1, 2), '--', 'color', [0 0 0 0.2], ...
       'DisplayName', '$RGA_{SVD}(i,j),\ i \neq j$');

  plot(freqs, RGA_svd(:, 1, 1), 'k-', ...
       'DisplayName', '$RGA_{SVD}(i,i)$');
  for ch_i = 1:6
    plot(freqs, RGA_svd(:, ch_i, ch_i), 'k-', ...
         'HandleVisibility', 'off');
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('Magnitude'); xlabel('Frequency [Hz]');
  legend('location', 'southwest');

  ax2 = nexttile;
  hold on;
  for i_in = 1:6
      for i_out = [1:i_in-1, i_in+1:6]
          plot(freqs, RGA_x(:, i_out, i_in), '--', 'color', [0 0 0 0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, RGA_x(:, 1, 2), '--', 'color', [0 0 0 0.2], ...
       'DisplayName', '$RGA_{X}(i,j),\ i \neq j$');

  plot(freqs, RGA_x(:, 1, 1), 'k-', ...
       'DisplayName', '$RGA_{X}(i,i)$');
  for ch_i = 1:6
    plot(freqs, RGA_x(:, ch_i, ch_i), 'k-', ...
         'HandleVisibility', 'off');
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  xlabel('Frequency [Hz]'); set(gca, 'YTickLabel',[]);
  legend('location', 'southwest');

  linkaxes([ax1,ax2],'y');
  ylim([1e-5, 1e1]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/simscape_model_rga.pdf', 'width', 'wide', 'height', 'tall');
#+end_src

#+name: fig:simscape_model_rga
#+caption: Obtained norm of RGA elements for the SVD decoupled plant and the Jacobian decoupled plant
#+RESULTS:
[[file:figs/simscape_model_rga.png]]

** Obtained Decoupled Plants
<<sec:stewart_decoupled_plant>>

The bode plot of the diagonal and off-diagonal elements of $G_{SVD}$ are shown in Figure [[fig:simscape_model_decoupled_plant_svd]].

#+begin_src matlab :exports none
  figure;
  tiledlayout(3, 1, 'TileSpacing', 'None', 'Padding', 'None');

  % Magnitude
  ax1 = nexttile([2, 1]);
  hold on;
  for i_in = 1:6
      for i_out = [1:i_in-1, i_in+1:6]
          plot(freqs, abs(squeeze(freqresp(Gsvd(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, abs(squeeze(freqresp(Gsvd(1, 2), freqs, 'Hz'))), 'color', [0,0,0,0.5], ...
       'DisplayName', '$G_{SVD}(i,j),\ i \neq j$');
  set(gca,'ColorOrderIndex',1)
  for ch_i = 1:6
    plot(freqs, abs(squeeze(freqresp(Gsvd(ch_i, ch_i), freqs, 'Hz'))), ...
         'DisplayName', sprintf('$G_{SVD}(%i,%i)$', ch_i, ch_i));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('Magnitude'); set(gca, 'XTickLabel',[]);
  legend('location', 'northwest');
  ylim([1e-1, 1e5])

  % Phase
  ax2 = nexttile;
  hold on;
  for ch_i = 1:6
    plot(freqs, 180/pi*angle(squeeze(freqresp(Gsvd(ch_i, ch_i), freqs, 'Hz'))));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'lin');
  ylabel('Phase [deg]'); xlabel('Frequency [Hz]');
  ylim([-180, 180]);
  yticks([-180:90:360]);

  linkaxes([ax1,ax2],'x');
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/simscape_model_decoupled_plant_svd.pdf', 'eps', true, 'width', 'wide', 'height', 'tall');
#+end_src

#+name: fig:simscape_model_decoupled_plant_svd
#+caption: Decoupled Plant using SVD
#+RESULTS:
[[file:figs/simscape_model_decoupled_plant_svd.png]]

Similarly, the bode plots of the diagonal elements and off-diagonal elements of the decoupled plant $G_x(s)$ using the Jacobian are shown in Figure [[fig:simscape_model_decoupled_plant_jacobian]].

#+begin_src matlab :exports none
  figure;
  tiledlayout(3, 1, 'TileSpacing', 'None', 'Padding', 'None');

  % Magnitude
  ax1 = nexttile([2, 1]);
  hold on;
  for i_in = 1:6
      for i_out = [1:i_in-1, i_in+1:6]
          plot(freqs, abs(squeeze(freqresp(Gx(i_out, i_in), freqs, 'Hz'))), 'color', [0,0,0,0.2], ...
               'HandleVisibility', 'off');
      end
  end
  plot(freqs, abs(squeeze(freqresp(Gx(1, 2), freqs, 'Hz'))), 'color', [0,0,0,0.5], ...
       'DisplayName', '$G_x(i,j),\ i \neq j$');
  set(gca,'ColorOrderIndex',1)
  plot(freqs, abs(squeeze(freqresp(Gx('Ax', 'Fx'), freqs, 'Hz'))), 'DisplayName', '$G_x(1,1) = A_x/F_x$');
  plot(freqs, abs(squeeze(freqresp(Gx('Ay', 'Fy'), freqs, 'Hz'))), 'DisplayName', '$G_x(2,2) = A_y/F_y$');
  plot(freqs, abs(squeeze(freqresp(Gx('Az', 'Fz'), freqs, 'Hz'))), 'DisplayName', '$G_x(3,3) = A_z/F_z$');
  plot(freqs, abs(squeeze(freqresp(Gx('Arx', 'Mx'), freqs, 'Hz'))), 'DisplayName', '$G_x(4,4) = A_{R_x}/M_x$');
  plot(freqs, abs(squeeze(freqresp(Gx('Ary', 'My'), freqs, 'Hz'))), 'DisplayName', '$G_x(5,5) = A_{R_y}/M_y$');
  plot(freqs, abs(squeeze(freqresp(Gx('Arz', 'Mz'), freqs, 'Hz'))), 'DisplayName', '$G_x(6,6) = A_{R_z}/M_z$');
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('Magnitude'); set(gca, 'XTickLabel',[]);
  legend('location', 'northwest');
  ylim([1e-2, 2e6])

  % Phase
  ax2 = nexttile;
  hold on;
  plot(freqs, 180/pi*angle(squeeze(freqresp(Gx('Ax', 'Fx'), freqs, 'Hz'))));
  plot(freqs, 180/pi*angle(squeeze(freqresp(Gx('Ay', 'Fy'), freqs, 'Hz'))));
  plot(freqs, 180/pi*angle(squeeze(freqresp(Gx('Az', 'Fz'), freqs, 'Hz'))));
  plot(freqs, 180/pi*angle(squeeze(freqresp(Gx('Arx', 'Mx'), freqs, 'Hz'))));
  plot(freqs, 180/pi*angle(squeeze(freqresp(Gx('Ary', 'My'), freqs, 'Hz'))));
  plot(freqs, 180/pi*angle(squeeze(freqresp(Gx('Arz', 'Mz'), freqs, 'Hz'))));
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'lin');
  ylabel('Phase [deg]'); xlabel('Frequency [Hz]');
  ylim([0, 180]);
  yticks([0:45:360]);

  linkaxes([ax1,ax2],'x');
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/simscape_model_decoupled_plant_jacobian.pdf', 'eps', true, 'width', 'wide', 'height', 'tall');
#+end_src

#+name: fig:simscape_model_decoupled_plant_jacobian
#+caption: Stewart Platform Plant from forces (resp. torques) applied by the legs to the acceleration (resp. angular acceleration) of the platform as well as all the coupling terms between the two (non-diagonal terms of the transfer function matrix)
#+RESULTS:
[[file:figs/simscape_model_decoupled_plant_jacobian.png]]

** Diagonal Controller
<<sec:stewart_diagonal_control>>
The control diagram for the centralized control is shown in Figure [[fig:centralized_control]].

The controller $K_c$ is "working" in an cartesian frame.
The Jacobian is used to convert forces in the cartesian frame to forces applied by the actuators.

#+begin_src latex :file centralized_control.pdf :tangle no :exports results
  \begin{tikzpicture}
    \node[block={2cm}{1.5cm}] (G) {$\begin{bmatrix}G_d\\G_u\end{bmatrix}$};
    \node[above] at (G.north) {$\bm{G}$};
    \node[block, below right=0.6 and -0.5 of G] (K) {$K_c$};
    \node[block, below left= 0.6 and -0.5 of G] (J) {$J^{-T}$};

    % Inputs of the controllers
    \coordinate[] (inputd) at ($(G.south west)!0.75!(G.north west)$);
    \coordinate[] (inputu) at ($(G.south west)!0.25!(G.north west)$);

    % Connections and labels
    \draw[<-] (inputd) -- ++(-0.8, 0) node[above right]{$D_w$};
    \draw[->] (G.east) -- ++(2.0, 0)  node[above left]{$a$};
    \draw[->] ($(G.east)+(1.4, 0)$)node[branch]{} |- (K.east);
    \draw[->] (K.west) -- (J.east) node[above right]{$\mathcal{F}$};
    \draw[->] (J.west) -- ++(-0.6, 0) |- (inputu) node[above left]{$\tau$};
  \end{tikzpicture}
#+end_src

#+name: fig:centralized_control
#+caption: Control Diagram for the Centralized control
#+RESULTS:
[[file:figs/centralized_control.png]]

The SVD control architecture is shown in Figure [[fig:svd_control]].
The matrices $U$ and $V$ are used to decoupled the plant $G$.

#+begin_src latex :file svd_control.pdf :tangle no :exports results
  \begin{tikzpicture}
    \node[block={2cm}{1.5cm}] (G) {$\begin{bmatrix}G_d\\G_u\end{bmatrix}$};
    \node[above] at (G.north) {$\bm{G}$};
    \node[block, below right=0.6 and 0 of G] (U) {$U^{-1}$};
    \node[block, below=0.6 of G] (K) {$K_{\text{SVD}}$};
    \node[block, below left= 0.6 and 0 of G] (V) {$V^{-T}$};

    % Inputs of the controllers
    \coordinate[] (inputd) at ($(G.south west)!0.75!(G.north west)$);
    \coordinate[] (inputu) at ($(G.south west)!0.25!(G.north west)$);

    % Connections and labels
    \draw[<-] (inputd) -- ++(-0.8, 0) node[above right]{$D_w$};
    \draw[->] (G.east) -- ++(2.5, 0) node[above left]{$a$};
    \draw[->] ($(G.east)+(2.0, 0)$) node[branch]{} |- (U.east);
    \draw[->] (U.west) -- (K.east);
    \draw[->] (K.west) -- (V.east);
    \draw[->] (V.west) -- ++(-0.6, 0) |- (inputu) node[above left]{$\tau$};
  \end{tikzpicture}
#+end_src

#+name: fig:svd_control
#+caption: Control Diagram for the SVD control
#+RESULTS:
[[file:figs/svd_control.png]]


We choose the controller to be a low pass filter:
\[ K_c(s) = \frac{G_0}{1 + \frac{s}{\omega_0}} \]

$G_0$ is tuned such that the crossover frequency corresponding to the diagonal terms of the loop gain is equal to $\omega_c$

#+begin_src matlab
  wc = 2*pi*80;  % Crossover Frequency [rad/s]
  w0 = 2*pi*0.1; % Controller Pole [rad/s]
#+end_src

#+begin_src matlab
  K_cen = diag(1./diag(abs(evalfr(Gx, j*wc))))*(1/abs(evalfr(1/(1 + s/w0), j*wc)))/(1 + s/w0);
  L_cen = K_cen*Gx;
  G_cen = feedback(G, pinv(J')*K_cen, [7:12], [1:6]);
#+end_src

#+begin_src matlab
  K_svd = diag(1./diag(abs(evalfr(Gsvd, j*wc))))*(1/abs(evalfr(1/(1 + s/w0), j*wc)))/(1 + s/w0);
  L_svd = K_svd*Gsvd;
  G_svd = feedback(G, inv(V')*K_svd*inv(U), [7:12], [1:6]);
#+end_src

The obtained diagonal elements of the loop gains are shown in Figure [[fig:stewart_comp_loop_gain_diagonal]].

#+begin_src matlab :exports none
  figure;
  tiledlayout(3, 1, 'TileSpacing', 'None', 'Padding', 'None');

  % Magnitude
  ax1 = nexttile([2, 1]);
  hold on;
  plot(freqs, abs(squeeze(freqresp(L_svd(1, 1), freqs, 'Hz'))), 'DisplayName', '$L_{SVD}(i,i)$');
  for i_in_out = 2:6
    set(gca,'ColorOrderIndex',1)
    plot(freqs, abs(squeeze(freqresp(L_svd(i_in_out, i_in_out), freqs, 'Hz'))), 'HandleVisibility', 'off');
  end

  set(gca,'ColorOrderIndex',2)
  plot(freqs, abs(squeeze(freqresp(L_cen(1, 1), freqs, 'Hz'))), ...
       'DisplayName', '$L_{J}(i,i)$');
  for i_in_out = 2:6
    set(gca,'ColorOrderIndex',2)
    plot(freqs, abs(squeeze(freqresp(L_cen(i_in_out, i_in_out), freqs, 'Hz'))), 'HandleVisibility', 'off');
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('Magnitude'); set(gca, 'XTickLabel',[]);
  legend('location', 'northwest');
  ylim([5e-2, 2e3])

  % Phase
  ax2 = nexttile;
  hold on;
  for i_in_out = 1:6
    set(gca,'ColorOrderIndex',1)
    plot(freqs, 180/pi*angle(squeeze(freqresp(L_svd(i_in_out, i_in_out), freqs, 'Hz'))));
  end
  set(gca,'ColorOrderIndex',2)
  for i_in_out = 1:6
    set(gca,'ColorOrderIndex',2)
    plot(freqs, 180/pi*angle(squeeze(freqresp(L_cen(i_in_out, i_in_out), freqs, 'Hz'))));
  end
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'lin');
  ylabel('Phase [deg]'); xlabel('Frequency [Hz]');
  ylim([-180, 180]);
  yticks([-180:90:360]);

  linkaxes([ax1,ax2],'x');
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/stewart_comp_loop_gain_diagonal.pdf', 'width', 'wide', 'height', 'tall');
#+end_src

#+name: fig:stewart_comp_loop_gain_diagonal
#+caption: Comparison of the diagonal elements of the loop gains for the SVD control architecture and the Jacobian one
#+RESULTS:
[[file:figs/stewart_comp_loop_gain_diagonal.png]]

** Closed-Loop system Performances
<<sec:stewart_closed_loop_results>>

Let's first verify the stability of the closed-loop systems:
#+begin_src matlab :results output replace text
  isstable(G_cen)
#+end_src

#+RESULTS:
: ans =
:   logical
:    1

#+begin_src matlab :results output replace text
  isstable(G_svd)
#+end_src

#+RESULTS:
: ans =
:   logical
:    1

The obtained transmissibility in Open-loop, for the centralized control as well as for the SVD control are shown in Figure [[fig:stewart_platform_simscape_cl_transmissibility]].

#+begin_src matlab :exports results
  figure;
  tiledlayout(2, 2, 'TileSpacing', 'None', 'Padding', 'None');

  ax1 = nexttile;
  hold on;
  plot(freqs, abs(squeeze(freqresp(G(    'Ax', 'Dwx')/s^2, freqs, 'Hz'))), 'DisplayName', 'Open-Loop');
  plot(freqs, abs(squeeze(freqresp(G_cen('Ax', 'Dwx')/s^2, freqs, 'Hz'))), 'DisplayName', 'Centralized');
  plot(freqs, abs(squeeze(freqresp(G_svd('Ax', 'Dwx')/s^2, freqs, 'Hz'))), '--', 'DisplayName', 'SVD');
  set(gca,'ColorOrderIndex',1)
  plot(freqs, abs(squeeze(freqresp(G(    'Ay', 'Dwy')/s^2, freqs, 'Hz'))), 'HandleVisibility', 'off');
  plot(freqs, abs(squeeze(freqresp(G_cen('Ay', 'Dwy')/s^2, freqs, 'Hz'))), 'HandleVisibility', 'off');
  plot(freqs, abs(squeeze(freqresp(G_svd('Ay', 'Dwy')/s^2, freqs, 'Hz'))), '--', 'HandleVisibility', 'off');
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('$D_x/D_{w,x}$, $D_y/D_{w, y}$'); set(gca, 'XTickLabel',[]);
  legend('location', 'southwest');

  ax2 = nexttile;
  hold on;
  plot(freqs, abs(squeeze(freqresp(G(    'Az', 'Dwz')/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_cen('Az', 'Dwz')/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_svd('Az', 'Dwz')/s^2, freqs, 'Hz'))), '--');
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('$D_z/D_{w,z}$'); set(gca, 'XTickLabel',[]);

  ax3 = nexttile;
  hold on;
  plot(freqs, abs(squeeze(freqresp(G(    'Arx', 'Rwx')/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_cen('Arx', 'Rwx')/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_svd('Arx', 'Rwx')/s^2, freqs, 'Hz'))), '--');
  set(gca,'ColorOrderIndex',1)
  plot(freqs, abs(squeeze(freqresp(G(    'Ary', 'Rwy')/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_cen('Ary', 'Rwy')/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_svd('Ary', 'Rwy')/s^2, freqs, 'Hz'))), '--');
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('$R_x/R_{w,x}$, $R_y/R_{w,y}$');  xlabel('Frequency [Hz]');

  ax4 = nexttile;
  hold on;
  plot(freqs, abs(squeeze(freqresp(G(    'Arz', 'Rwz')/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_cen('Arz', 'Rwz')/s^2, freqs, 'Hz'))));
  plot(freqs, abs(squeeze(freqresp(G_svd('Arz', 'Rwz')/s^2, freqs, 'Hz'))), '--');
  hold off;
  set(gca, 'XScale', 'log'); set(gca, 'YScale', 'log');
  ylabel('$R_z/R_{w,z}$');  xlabel('Frequency [Hz]');

  linkaxes([ax1,ax2,ax3,ax4],'xy');
  xlim([freqs(1), freqs(end)]);
  ylim([1e-3, 1e2]);
#+end_src

#+begin_src matlab :tangle no :exports results :results file replace
  exportFig('figs/stewart_platform_simscape_cl_transmissibility.pdf', 'eps', true, 'width', 'wide', 'height', 'tall');
#+end_src

#+name: fig:stewart_platform_simscape_cl_transmissibility
#+caption: Obtained Transmissibility
#+RESULTS:
[[file:figs/stewart_platform_simscape_cl_transmissibility.png]]

