+++
title = "Connectors"
author = ["Thomas Dehaeze"]
draft = false
+++

Tags
: [Cables]({{< relref "cables" >}})


## Manufacturers {#manufacturers}

| Manufacturers                                      | Country     |
|----------------------------------------------------|-------------|
| [LEMO](https://www.lemo.com/en)                    | Switzerland |
| [Fischer](https://www.fischerconnectors.com/uk/en) | Switzerland |
| [EDO](https://www.odu-connectors.com/)             | Germany     |


## BNC {#bnc}

BNC connectors can have an impedance of 50Ohms or 75Ohms as shown in Figure [1](#orgd1b23d3).

<a id="orgd1b23d3"></a>

{{< figure src="/ox-hugo/bnc_50_75_ohms.jpg" caption="Figure 1: 75Ohms and 50Ohms BNC connectors" >}}
